<map id="RFIDManagerInit" name="RFIDManagerInit">
<area shape="rect" id="node2" href="$_c_r95_h_f_8c.html#a5a280da3bb75613fbb5e62854ec65e3a" title="Function used to initialize the CR95HF global manager. " alt="" coords="173,107,261,133"/>
<area shape="rect" id="node3" href="$_c_r95_uart_mapper_8c.html#a530fdd7929335f4103bf44a111d9f441" title="CR95HF Uart interface. " alt="" coords="310,107,405,133"/>
<area shape="rect" id="node4" href="$uart0_8c.html#a2ed82ee365da2b37ca2446c607b38a4e" title="Initialize this uart. " alt="" coords="471,56,542,83"/>
<area shape="rect" id="node7" href="$uart2_8c.html#aa5a4b7bf2a92075993a2f8a8b5b0bdf6" title="Initialize this uart. " alt="" coords="471,107,542,133"/>
<area shape="rect" id="node10" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="453,157,560,184"/>
<area shape="rect" id="node5" href="$_d_s_p__mkl16z256vlh4_8c.html#aa0ebd2465a6d7946e08a90b6dd0dfd90" title="Functions to enable/disable the main clock of the specified uart. " alt="" coords="641,5,765,32"/>
<area shape="rect" id="node6" href="$_d_s_p__mkl16z256vlh4_8c.html#a31b8687080bee1920824bf09eadcf072" title="Functions to MAP the defined IO of the uart module x in the rigth pin. " alt="" coords="608,56,797,83"/>
<area shape="rect" id="node8" href="$_d_s_p__mkl16z256vlh4_8c.html#aaf402774cc148a8964baef5dfa2c0f63" title="UART2ClockGate" alt="" coords="641,107,765,133"/>
<area shape="rect" id="node9" href="$_d_s_p__mkl16z256vlh4_8c.html#ad0a54c089f47188bd51d40aa13094b70" title="UART2PinMappingPeripheral" alt="" coords="608,157,797,184"/>
</map>
