<map id="PowerManagerEnterLPM" name="PowerManagerEnterLPM">
<area shape="rect" id="node2" href="$display_8c.html#a20d8e5860540ecfe3c0bb5a237bc17f8" title="Function used to enable/disable the display power. " alt="" coords="261,17,382,44"/>
<area shape="rect" id="node4" href="$_f_m25_v20_8c.html#ab71cea0f2db62d709c9b1a6441a70581" title="Put the memory in a low power mode. " alt="" coords="269,80,374,107"/>
<area shape="rect" id="node6" href="$device_8c.html#afc4edee1a81067e2cd15de38145be61e" title="Function to switch the device in very low power mode. " alt="" coords="276,131,367,157"/>
<area shape="rect" id="node8" href="$_power_manager_8c.html#a841a006cab2c35f157e9cb986a5ed4cf" title="Functions used to control the wake up interrupt functions. " alt="" coords="222,182,421,223"/>
<area shape="rect" id="node10" href="$_d_s_p__mkl16z256vlh4_8c.html#aa0ebd2465a6d7946e08a90b6dd0dfd90" title="Functions to enable/disable the main clock of the specified uart. " alt="" coords="259,248,383,275"/>
<area shape="rect" id="node11" href="$_d_s_p__mkl16z256vlh4_8c.html#ade83ccc4c990b0da74572b7fbc556015" title="UART1ClockGate" alt="" coords="259,299,383,325"/>
<area shape="rect" id="node12" href="$_d_s_p__mkl16z256vlh4_8c.html#aaf402774cc148a8964baef5dfa2c0f63" title="UART2ClockGate" alt="" coords="259,349,383,376"/>
<area shape="rect" id="node13" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="268,400,375,427"/>
<area shape="rect" id="node3" href="$_d_s_p__mkl16z256vlh4_8c.html#ad30b60ccfc1302cb250629c495851333" title="Functions to MAP the defined IO of the SPI module x in the rigth pin. " alt="" coords="512,5,688,32"/>
<area shape="rect" id="node5" href="$spi1_8c.html#a3d9bbade5a2bc2bfbc959fa5520cf3e0" title="Function used to send data over the SPI module 1. " alt="" coords="561,80,639,107"/>
<area shape="rect" id="node7" href="$device_8c.html#a377a70c9537e7f7cff20ba3e7205264a" title="Function to switch the device in deep sleep mode. " alt="" coords="541,131,659,157"/>
<area shape="rect" id="node9" href="$_power_manager_8c.html#ad82283ab9a30920f56833e7d42dd66c8" title="PowerManagerClearWakeUpInterruptFlag" alt="" coords="470,189,730,216"/>
</map>
