SRD Standelone programmation box: tFM25V20StatusReg Union Reference

| SRD Standelone programmation box 2.0 (16/11/15 10:00:00) Documentation of the SRD standelone programmation box

- Main Page
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Enumerations Enumerator Macros Pages
Data Fields
tFM25V20StatusReg Union Reference

structure used to read and get the status register of the device. More...

`#include "FM25V20.h"`

## Data Fields

struct {
unsigned char RSVD0: 1
unsigned char WEL: 1
unsigned char BP0: 1
unsigned char BP1: 1
unsigned char RSVD1: 3
unsigned char WPEN: 1
} | bits
unsigned char | all

## Detailed Description

structure used to read and get the status register of the device.

Definition at line 132 of file FM25V20.h.

## Field Documentation

unsigned char tFM25V20StatusReg::all

global access

Definition at line 141 of file FM25V20.h.

Referenced by FM25V20ReadStatusReg(), and FM25V20SetStatusReg().

struct { ... } tFM25V20StatusReg::bits

bit access

Referenced by FM25V20Init().

unsigned char tFM25V20StatusReg::BP0

BP0 bit

Definition at line 136 of file FM25V20.h.

Referenced by FM25V20Init().

unsigned char tFM25V20StatusReg::BP1

BP1 bit

Definition at line 137 of file FM25V20.h.

Referenced by FM25V20Init().

unsigned char tFM25V20StatusReg::RSVD0

RESERVED

Definition at line 134 of file FM25V20.h.

unsigned char tFM25V20StatusReg::RSVD1

RESERVED

Definition at line 138 of file FM25V20.h.

unsigned char tFM25V20StatusReg::WEL

WEL bit

Definition at line 135 of file FM25V20.h.

unsigned char tFM25V20StatusReg::WPEN

WPEN bit

Definition at line 139 of file FM25V20.h.

Referenced by FM25V20Init().

The documentation for this union was generated from the following file:

- FM25V20.h