<map id="CR95UartInit" name="CR95UartInit">
<area shape="rect" id="node2" href="$uart0_8c.html#a2ed82ee365da2b37ca2446c607b38a4e" title="Initialize this uart. " alt="" coords="167,56,238,83"/>
<area shape="rect" id="node5" href="$uart2_8c.html#aa5a4b7bf2a92075993a2f8a8b5b0bdf6" title="Initialize this uart. " alt="" coords="167,107,238,133"/>
<area shape="rect" id="node8" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="149,157,256,184"/>
<area shape="rect" id="node3" href="$_d_s_p__mkl16z256vlh4_8c.html#aa0ebd2465a6d7946e08a90b6dd0dfd90" title="Functions to enable/disable the main clock of the specified uart. " alt="" coords="337,5,461,32"/>
<area shape="rect" id="node4" href="$_d_s_p__mkl16z256vlh4_8c.html#a31b8687080bee1920824bf09eadcf072" title="Functions to MAP the defined IO of the uart module x in the rigth pin. " alt="" coords="304,56,493,83"/>
<area shape="rect" id="node6" href="$_d_s_p__mkl16z256vlh4_8c.html#aaf402774cc148a8964baef5dfa2c0f63" title="UART2ClockGate" alt="" coords="337,107,461,133"/>
<area shape="rect" id="node7" href="$_d_s_p__mkl16z256vlh4_8c.html#ad0a54c089f47188bd51d40aa13094b70" title="UART2PinMappingPeripheral" alt="" coords="304,157,493,184"/>
</map>
