<map id="Uart0Init" name="Uart0Init">
<area shape="rect" id="node2" href="$_d_s_p__mkl16z256vlh4_8c.html#aa0ebd2465a6d7946e08a90b6dd0dfd90" title="Functions to enable/disable the main clock of the specified uart. " alt="" coords="158,5,282,32"/>
<area shape="rect" id="node3" href="$_d_s_p__mkl16z256vlh4_8c.html#a31b8687080bee1920824bf09eadcf072" title="Functions to MAP the defined IO of the uart module x in the rigth pin. " alt="" coords="125,56,315,83"/>
</map>
