<map id="ButtonManager" name="ButtonManager">
<area shape="rect" id="node2" href="$_button_manager_8c.html#afdd019b240e44a51aba9069b09cd3ee8" title="ButtonManagerDealer" alt="" coords="184,480,331,506"/>
<area shape="rect" id="node14" href="$display_8c.html#a20d8e5860540ecfe3c0bb5a237bc17f8" title="Function used to enable/disable the display power. " alt="" coords="717,365,838,392"/>
<area shape="rect" id="node16" href="$display_8c.html#a0529c896e4069df4bb7c4e767f36be28" title="Function used set the data displayed. " alt="" coords="693,256,862,282"/>
<area shape="rect" id="node22" href="$tick_8c.html#aa43bd4bc67b26f7e7ab31be06b088a14" title="Get the milliseconds counter. " alt="" coords="712,765,843,792"/>
<area shape="rect" id="node27" href="$tick_8c.html#a0145cffb9b0238336157774cbdb484a9" title="Get the milliseconds counter. " alt="" coords="426,714,595,741"/>
<area shape="rect" id="node28" href="$_button_manager_8c.html#a72f46a32970390d2c24e0e177d3d7985" title="ButtonManagerDisplayDate\lError" alt="" coords="421,110,601,151"/>
<area shape="rect" id="node29" href="$_button_manager_8c.html#a46d3f9715cc22d9bb745d0971b137094" title="ButtonManagerDisplayNone" alt="" coords="419,176,602,202"/>
<area shape="rect" id="node30" href="$_button_manager_8c.html#ac9681c8a673eea2c004dcd6838accb03" title="ButtonManagerDisplayProgrammed\lError" alt="" coords="397,44,624,86"/>
<area shape="rect" id="node31" href="$display_8c.html#ad8f9098d6f81dbce9ff70ef99662f212" title="Function used get the data displayed. " alt="" coords="172,816,343,842"/>
<area shape="rect" id="node32" href="$rtc_8c.html#acc23a8b28879660bbc371e432dd1c140" title="Indicate if the RTC have been initialized or not. " alt="" coords="166,866,349,893"/>
<area shape="rect" id="node3" href="$_memory_manager_8c.html#aaf68fcb13458866a83fe16fa9c66aca9" title="function used read/write and check the log in the memory. " alt="" coords="425,613,596,640"/>
<area shape="rect" id="node12" href="$rtc_8c.html#a12763edd744e1e2eb152fc965e0705d6" title="return the current time in the RTC. " alt="" coords="465,226,556,253"/>
<area shape="rect" id="node13" href="$_button_manager_8c.html#ab2d0aabb7a374961991dd4a80c0c9654" title="ButtonManagerDisplayRfid\lError" alt="" coords="423,328,598,370"/>
<area shape="rect" id="node23" href="$_button_manager_8c.html#a9e4446b1a305b75138f80df13ca38f26" title="ButtonManagerDisplayLogError" alt="" coords="409,394,612,421"/>
<area shape="rect" id="node24" href="$_button_manager_8c.html#a7467a0fb45a4b96ba5e07000b94aaeea" title="ButtonManagerDisplayWrite\lError" alt="" coords="419,446,603,487"/>
<area shape="rect" id="node25" href="$_button_manager_8c.html#ae2f1b19b0a4b64760e2fe56761fadb76" title="ButtonManagerDisplayWrite" alt="" coords="419,512,603,538"/>
<area shape="rect" id="node26" href="$_button_manager_8c.html#a9afe02c03b610c40e5d86a88873f0b65" title="ButtonManagerDisplayRead" alt="" coords="419,277,602,304"/>
<area shape="rect" id="node4" href="$checksum_8c.html#aea3900f8f3c22134b50fbb7fe78a487b" title="ChecksumByteOnShortCompute" alt="" coords="672,512,883,538"/>
<area shape="rect" id="node5" href="$_f_m25_v20_8c.html#adb5842f7204713f99fa6ce183317a523" title="Get the low power status of the memory. " alt="" coords="699,562,856,589"/>
<area shape="rect" id="node6" href="$_f_m25_v20_8c.html#a3866b69abe44cb40d09f89c2cc3ba8b3" title="Wake up the memory from the low power mode. " alt="" coords="713,613,841,640"/>
<area shape="rect" id="node7" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="724,664,831,690"/>
<area shape="rect" id="node8" href="$_f_m25_v20_8c.html#a614bc8a001d6845b564f529dc542410d" title="Write data to the memory. " alt="" coords="709,714,845,741"/>
<area shape="rect" id="node11" href="$_f_m25_v20_8c.html#ab71cea0f2db62d709c9b1a6441a70581" title="Put the memory in a low power mode. " alt="" coords="966,514,1071,541"/>
<area shape="rect" id="node9" href="$_f_m25_v20_8c.html#addeb196cb46ebc29e8f5e59e8dd01b15" title="Function used to set the write mode. " alt="" coords="931,664,1107,690"/>
<area shape="rect" id="node10" href="$spi1_8c.html#a3d9bbade5a2bc2bfbc959fa5520cf3e0" title="Function used to send data over the SPI module 1. " alt="" coords="1155,664,1234,690"/>
<area shape="rect" id="node15" href="$_d_s_p__mkl16z256vlh4_8c.html#ad30b60ccfc1302cb250629c495851333" title="Functions to MAP the defined IO of the SPI module x in the rigth pin. " alt="" coords="931,398,1107,425"/>
<area shape="rect" id="node17" href="$display_8c.html#ace411722dfe7b549d16c09991a5ff24f" title="Function used to root 7 segments command on the rigth PIN. " alt="" coords="951,348,1086,374"/>
<area shape="rect" id="node18" href="$decoder7_seg_8c.html#a8e8cab35cf7c9517f7094f42637a086e" title="Function used to decode a char and display it on a 7 segments digit. " alt="" coords="942,121,1095,148"/>
<area shape="rect" id="node19" href="$display_8c.html#a771439bf50110fb999649ac3262bc4ef" title="Function used to root 16 segments command on the rigth PIN. " alt="" coords="947,172,1090,198"/>
<area shape="rect" id="node20" href="$decoder16_seg_8c.html#a2d2fc41a03a66256e4681e8d695f01b0" title="Function used to decode a char and display it on a 16 segments digit. " alt="" coords="939,222,1099,249"/>
<area shape="rect" id="node21" href="$spi0_8c.html#a6d528a26e3df5e8bdb80622df3946998" title="Function used to send data over the SPI module 0. " alt="" coords="979,297,1058,324"/>
</map>
