<map id="RFIDDealer" name="RFIDDealer">
<area shape="rect" id="node2" href="$_r_f_i_d_manager_8c.html#a6ab6b8dd0e473d8fdf4a01c3ffbd7852" title="RFIDBridgeStateMachine" alt="" coords="145,537,313,564"/>
<area shape="rect" id="node17" href="$_r_f_i_d_manager_8c.html#aaadf0da29bf3176eb69c6e8ec6e08a6b" title="RFIDExtLpmStateMachine" alt="" coords="141,765,317,792"/>
<area shape="rect" id="node20" href="$_r_f_i_d_manager_8c.html#a76aaad614e4215dd0b1f0a55c91448ff" title="RFIDIntLpmStateMachine" alt="" coords="144,816,315,843"/>
<area shape="rect" id="node21" href="$_r_f_i_d_manager_8c.html#a776bd19e29a44fe5b562330efe4b1808" title="RFIDReadStateMachine" alt="" coords="149,411,310,437"/>
<area shape="rect" id="node23" href="$_r_f_i_d_manager_8c.html#aa800930fc21149f77f2b93ece7ede47b" title="RFIDWriteStateMachine" alt="" coords="148,309,311,336"/>
<area shape="rect" id="node3" href="$_c_r95_uart_mapper_8c.html#a7ad185503043b02e75769ae9ebb3e6b9" title="Return the connection state of the CR95HF module. " alt="" coords="375,309,566,336"/>
<area shape="rect" id="node4" href="$_c_r95_h_f_8c.html#a652e787d25427bedbd66533629298f5a" title="Return the current state of the CR95HF module in it&#39;s manager. " alt="" coords="387,816,555,843"/>
<area shape="rect" id="node5" href="$_c_r95_h_f_8c.html#ab73c2e7ae98f669c93c235a762f27649" title="CR95HFStartBridge" alt="" coords="403,613,539,640"/>
<area shape="rect" id="node6" href="$_c_r95_h_f_8c.html#af52d793b7c0dbefdfa0b2060f0366a3d" title="Manager used to deal each specific state. " alt="" coords="406,765,535,792"/>
<area shape="rect" id="node7" href="$_c_r95_h_f_8c.html#a27506223088d2179f105cc721bd17d99" title="CR95HFStartField15693" alt="" coords="389,411,552,437"/>
<area shape="rect" id="node8" href="$_c_r95_uart_mapper_8c.html#ae9b7dcc01097b34d264ecc59cfd3659e" title="Select the antenna used to communicate with the SRD. " alt="" coords="406,512,535,539"/>
<area shape="rect" id="node9" href="$_c_r95_uart_mapper_8c.html#a073808c89f3a15ef8044992f7ec9ccdb" title="CR95UartDisableReceiver" alt="" coords="385,360,556,387"/>
<area shape="rect" id="node10" href="$_c_r95_uart_mapper_8c.html#aa48280ff1cfa4743c04d90e8b18c7144" title="CR95UartSendData" alt="" coords="403,208,538,235"/>
<area shape="rect" id="node13" href="$tick_8c.html#aa43bd4bc67b26f7e7ab31be06b088a14" title="Get the milliseconds counter. " alt="" coords="624,360,755,387"/>
<area shape="rect" id="node14" href="$tick_8c.html#a0145cffb9b0238336157774cbdb484a9" title="Get the milliseconds counter. " alt="" coords="386,259,555,285"/>
<area shape="rect" id="node15" href="$_usb_manager_8c.html#a3faf19ddc73b0a9e25c5b66dd5b49bff" title="Function used to send the CR95 error on the USB. " alt="" coords="378,715,563,741"/>
<area shape="rect" id="node16" href="$_usb_manager_8c.html#a9246dcc92e2a78422be0a94688fcf853" title="Function used to send the CR95 result of last RFID operation on the USB. " alt="" coords="373,563,568,589"/>
<area shape="rect" id="node11" href="$uart0_8c.html#a702d354b2f7a798728f7b564c6a5bc35" title="send data other uart. " alt="" coords="634,183,745,209"/>
<area shape="rect" id="node12" href="$uart2_8c.html#abc17789ee9265fd32a53f68b0c16d2d8" title="send data other uart. " alt="" coords="634,233,745,260"/>
<area shape="rect" id="node18" href="$_c_r95_h_f_8c.html#a1291f99a43efc55ba45a58ffb5899c8e" title="CR95HFStartFieldOff" alt="" coords="399,867,542,893"/>
<area shape="rect" id="node19" href="$_c_r95_h_f_8c.html#a35fb88e6119a4cfa8f0014973f6339ce" title="CR95HFStartHibernate" alt="" coords="393,917,548,944"/>
<area shape="rect" id="node22" href="$_c_r95_h_f_8c.html#ae8388513b3c386e588c3539aded54006" title="CR95HFStartRead" alt="" coords="406,157,535,184"/>
<area shape="rect" id="node24" href="$_c_r95_h_f_8c.html#aba2c35a53fa89e7805a8513d98981a69" title="CR95HFStartWrite" alt="" coords="405,56,536,83"/>
<area shape="rect" id="node25" href="$checksum_8c.html#aea3900f8f3c22134b50fbb7fe78a487b" title="ChecksumByteOnShortCompute" alt="" coords="365,5,576,32"/>
</map>
