SRD Standelone programmation box: tUartCtrl Union Reference

| SRD Standelone programmation box 2.0 (16/11/15 10:00:00) Documentation of the SRD standelone programmation box

- Main Page
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Enumerations Enumerator Macros Pages
Data Fields
tUartCtrl Union Reference

Define the Uart control structure. More...

`#include "uart_common.h"`

Collaboration diagram for tUartCtrl:
[legend]

## Data Fields

tUartFifo | rx
tUartFifo | tx
tUartFlags | flags

## Detailed Description

Define the Uart control structure.

Definition at line 76 of file uart_common.h.

## Field Documentation

tUartFlags tUartCtrl::flags

Flags

Definition at line 79 of file uart_common.h.

Referenced by CR95UartResetReceiver(), UART0_IRQHandler(), Uart0Init(), Uart0ReadChar(), Uart0SendData(), Uart0SendString(), UART1_IRQHandler(), Uart1Init(), Uart1ReadChar(), Uart1SendData(), Uart1SendString(), UART2_IRQHandler(), Uart2Init(), Uart2ReadChar(), Uart2SendData(), and Uart2SendString().

tUartFifo tUartCtrl::rx

Rx FIFO

Definition at line 77 of file uart_common.h.

Referenced by CR95HFReadAnswer(), CR95UartResetReceiver(), UART0_IRQHandler(), Uart0Init(), Uart0ReadChar(), UART1_IRQHandler(), Uart1Init(), Uart1ReadChar(), UART2_IRQHandler(), Uart2Init(), and Uart2ReadChar().

tUartFifo tUartCtrl::tx

Tx FIFO

Definition at line 78 of file uart_common.h.

Referenced by UART0_IRQHandler(), Uart0Init(), Uart0SendData(), Uart0SendString(), UART1_IRQHandler(), Uart1Init(), Uart1SendData(), Uart1SendString(), UART2_IRQHandler(), Uart2Init(), Uart2SendData(), and Uart2SendString().

The documentation for this union was generated from the following file:

- uart_common.h