<map id="PowerManagerLPMController" name="PowerManagerLPMController">
<area shape="rect" id="node2" href="$_power_manager_8c.html#a7406ccf39ad8768c5043ac74da94a63b" title="Functions used to Enter and exit low power mode. " alt="" coords="246,670,413,697"/>
<area shape="rect" id="node15" href="$_power_manager_8c.html#a1c56b577113fb8580a4f6fb0abe50fea" title="PowerManagerExitLPM" alt="" coords="250,797,409,824"/>
<area shape="rect" id="node3" href="$display_8c.html#a20d8e5860540ecfe3c0bb5a237bc17f8" title="Function used to enable/disable the display power. " alt="" coords="1069,1024,1190,1050"/>
<area shape="rect" id="node5" href="$_f_m25_v20_8c.html#ab71cea0f2db62d709c9b1a6441a70581" title="Put the memory in a low power mode. " alt="" coords="510,417,615,444"/>
<area shape="rect" id="node7" href="$device_8c.html#afc4edee1a81067e2cd15de38145be61e" title="Function to switch the device in very low power mode. " alt="" coords="517,473,608,500"/>
<area shape="rect" id="node9" href="$_power_manager_8c.html#a841a006cab2c35f157e9cb986a5ed4cf" title="Functions used to control the wake up interrupt functions. " alt="" coords="463,534,662,575"/>
<area shape="rect" id="node11" href="$_d_s_p__mkl16z256vlh4_8c.html#aa0ebd2465a6d7946e08a90b6dd0dfd90" title="Functions to enable/disable the main clock of the specified uart. " alt="" coords="501,721,625,748"/>
<area shape="rect" id="node12" href="$_d_s_p__mkl16z256vlh4_8c.html#ade83ccc4c990b0da74572b7fbc556015" title="UART1ClockGate" alt="" coords="501,772,625,798"/>
<area shape="rect" id="node13" href="$_d_s_p__mkl16z256vlh4_8c.html#aaf402774cc148a8964baef5dfa2c0f63" title="UART2ClockGate" alt="" coords="501,620,625,646"/>
<area shape="rect" id="node14" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="509,670,616,697"/>
<area shape="rect" id="node4" href="$_d_s_p__mkl16z256vlh4_8c.html#ad30b60ccfc1302cb250629c495851333" title="Functions to MAP the defined IO of the SPI module x in the rigth pin. " alt="" coords="1285,1104,1461,1130"/>
<area shape="rect" id="node6" href="$spi1_8c.html#a3d9bbade5a2bc2bfbc959fa5520cf3e0" title="Function used to send data over the SPI module 1. " alt="" coords="803,412,882,438"/>
<area shape="rect" id="node8" href="$device_8c.html#a377a70c9537e7f7cff20ba3e7205264a" title="Function to switch the device in deep sleep mode. " alt="" coords="783,462,902,489"/>
<area shape="rect" id="node10" href="$_power_manager_8c.html#ad82283ab9a30920f56833e7d42dd66c8" title="PowerManagerClearWakeUpInterruptFlag" alt="" coords="713,513,973,540"/>
<area shape="rect" id="node16" href="$device_8c.html#a631a644dd7e158b7fa45c4bfe43b29bc" title="Function to switch the processor on the highest clock speed allowed. " alt="" coords="465,986,660,1013"/>
<area shape="rect" id="node17" href="$_power_manager_8c.html#a611c841c363bb8044e88747cc39e7c30" title="power manager. " alt="" coords="509,873,617,900"/>
<area shape="rect" id="node49" href="$_power_manager_8c.html#abc288b84841dcde78bcdb6f57da9d8d1" title="PowerManagerDisableWakeUp\lInterrupt" alt="" coords="462,1038,663,1079"/>
<area shape="rect" id="node18" href="$_b_q27510_d_r_z_r_g2_8c.html#ab6764798c058c46b3cdcf21c97027ffb" title="Function used to get all information about the cell monitoring. " alt="" coords="789,564,896,590"/>
<area shape="rect" id="node39" href="$_power_manager_8c.html#a851ecff0a5e93c3b261accadbf32621b" title="PowerManagerDisplayLoaded" alt="" coords="746,860,939,886"/>
<area shape="rect" id="node47" href="$_power_manager_8c.html#aa781287c32b2238935eb53a6ce806419" title="PowerManagerDisplayLoading" alt="" coords="745,910,941,937"/>
<area shape="rect" id="node48" href="$_power_manager_8c.html#a20ccb5a44ea9c3ecb98d6ec3ed84c62a" title="PowerManagerDisplayLoading\lError" alt="" coords="745,962,941,1003"/>
<area shape="rect" id="node19" href="$_b_q27510_d_r_z_r_g2_8c.html#ab9dcad56c77f04971532555567a0d84b" title="Function used to know if a battery is connected or not. " alt="" coords="1293,184,1453,210"/>
<area shape="rect" id="node21" href="$_b_q27510_d_r_z_r_g2_8c.html#ac5d4fef49e298779b1753f40cf601cd3" title="BQ_getAvailableEnergy" alt="" coords="1050,462,1209,489"/>
<area shape="rect" id="node23" href="$_b_q27510_d_r_z_r_g2_8c.html#a9854bebed505691984f1cfa674cb3cb1" title="BQ_getAverageCurrent" alt="" coords="1052,513,1207,540"/>
<area shape="rect" id="node24" href="$_b_q27510_d_r_z_r_g2_8c.html#a28acfc3f3d1ff8e9d9d91edadc29ecd5" title="BQ_getAveragePower" alt="" coords="1055,564,1203,590"/>
<area shape="rect" id="node25" href="$_b_q27510_d_r_z_r_g2_8c.html#af8268e396eeb7abdfb21a7fbf03f1396" title="Function used to get some information about the cell monitoring. " alt="" coords="1049,614,1209,641"/>
<area shape="rect" id="node26" href="$_b_q27510_d_r_z_r_g2_8c.html#af6d8cc1ca065bcb90798788851de572c" title="BQ_getCellVoltage" alt="" coords="1063,665,1195,692"/>
<area shape="rect" id="node27" href="$_b_q27510_d_r_z_r_g2_8c.html#a02b013ae0aec405f9c7ceb909199f5f0" title="BQ_getCycleCount" alt="" coords="1063,716,1196,742"/>
<area shape="rect" id="node28" href="$_b_q27510_d_r_z_r_g2_8c.html#aaead900b00cb48e635c7db154f99c3e5" title="BQ_getFullAvailableCapacity" alt="" coords="1035,766,1224,793"/>
<area shape="rect" id="node29" href="$_b_q27510_d_r_z_r_g2_8c.html#a148f18dc993b083cacc31ff1f4dc71ed" title="BQ_getFullChargeCapacity" alt="" coords="1040,817,1219,844"/>
<area shape="rect" id="node30" href="$_b_q27510_d_r_z_r_g2_8c.html#a42dac1127d0914053de05fd9af45b77a" title="BQ_getMaxLoadCurrent" alt="" coords="1049,868,1210,894"/>
<area shape="rect" id="node31" href="$_b_q27510_d_r_z_r_g2_8c.html#aa723c8cc7b39b74ae4c344cb39350aed" title="BQ_getMaxLoadTimeToEmpty" alt="" coords="1030,57,1229,84"/>
<area shape="rect" id="node32" href="$_b_q27510_d_r_z_r_g2_8c.html#a14b533c028c320fc9b2a5b9043d0e259" title="BQ_getNominalAvailableCapacity" alt="" coords="1022,108,1237,134"/>
<area shape="rect" id="node33" href="$_b_q27510_d_r_z_r_g2_8c.html#a6602062ce84e9142bfab316784516eb8" title="BQ_getRemainingCapacity" alt="" coords="1040,158,1219,185"/>
<area shape="rect" id="node34" href="$_b_q27510_d_r_z_r_g2_8c.html#a3a21f0765f44c716b638d8b8773946d2" title="BQ_getStandbyTimeToEmpty" alt="" coords="1032,209,1227,236"/>
<area shape="rect" id="node35" href="$_b_q27510_d_r_z_r_g2_8c.html#a84d862a65a34dff063b11338b89a5931" title="BQ_getStateOfCharge" alt="" coords="1054,260,1205,286"/>
<area shape="rect" id="node36" href="$_b_q27510_d_r_z_r_g2_8c.html#ab0c39d16ad675e6a83e2659c9a51551b" title="BQ_getTimeToEmpty" alt="" coords="1056,310,1203,337"/>
<area shape="rect" id="node37" href="$_b_q27510_d_r_z_r_g2_8c.html#aade4e442c60a3cf1aa9223a7696483dc" title="BQ_getTimeToFull" alt="" coords="1065,361,1194,388"/>
<area shape="rect" id="node38" href="$_b_q27510_d_r_z_r_g2_8c.html#a8a62d091a91f6665acc0bd38ee9af9da" title="BQ_getTTEAtConstantPower" alt="" coords="1034,412,1225,438"/>
<area shape="rect" id="node20" href="$i2c0_8c.html#ada7d730a8793a6ddd23180047b309447" title="Send a packet on the I2C interface. " alt="" coords="1510,310,1589,337"/>
<area shape="rect" id="node22" href="$i2c0_8c.html#a1f3862c3506c31b0a50c7914f17314ab" title="Read a packet on the I2C interface. " alt="" coords="1334,437,1413,464"/>
<area shape="rect" id="node40" href="$display_8c.html#ad8f9098d6f81dbce9ff70ef99662f212" title="Function used get the data displayed. " alt="" coords="1044,918,1215,945"/>
<area shape="rect" id="node41" href="$display_8c.html#a0529c896e4069df4bb7c4e767f36be28" title="Function used set the data displayed. " alt="" coords="1045,969,1214,996"/>
<area shape="rect" id="node42" href="$decoder16_seg_8c.html#a2d2fc41a03a66256e4681e8d695f01b0" title="Function used to decode a char and display it on a 16 segments digit. " alt="" coords="1293,1053,1453,1080"/>
<area shape="rect" id="node43" href="$decoder7_seg_8c.html#a8e8cab35cf7c9517f7094f42637a086e" title="Function used to decode a char and display it on a 7 segments digit. " alt="" coords="1297,826,1450,853"/>
<area shape="rect" id="node44" href="$display_8c.html#a771439bf50110fb999649ac3262bc4ef" title="Function used to root 16 segments command on the rigth PIN. " alt="" coords="1302,877,1445,904"/>
<area shape="rect" id="node45" href="$display_8c.html#ace411722dfe7b549d16c09991a5ff24f" title="Function used to root 7 segments command on the rigth PIN. " alt="" coords="1306,928,1441,954"/>
<area shape="rect" id="node46" href="$spi0_8c.html#a6d528a26e3df5e8bdb80622df3946998" title="Function used to send data over the SPI module 0. " alt="" coords="1334,1002,1413,1029"/>
</map>
