<map id="MemoryManagerInit" name="MemoryManagerInit">
<area shape="rect" id="node2" href="$_f_m25_v20_8c.html#a2e18e393748dca1da43e4e069bc4972f" title="Function used to initialize the FM25V20 memory. " alt="" coords="249,132,343,159"/>
<area shape="rect" id="node9" href="$_memory_manager_8c.html#a23afd9881c251d81c7ff88b4fefbb8e4" title="MemoryManagerCheckDiving" alt="" coords="201,524,391,551"/>
<area shape="rect" id="node11" href="$_memory_manager_8c.html#a7b3973e4132860fb79b75c73bc111a6f" title="MemoryManagerCheckSerial" alt="" coords="201,473,391,500"/>
<area shape="rect" id="node12" href="$_memory_manager_8c.html#a95c0f9ae110105c19fb6eb0da09930e0" title="Return the number of log stored in memory. " alt="" coords="190,271,402,297"/>
<area shape="rect" id="node18" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="479,423,585,449"/>
<area shape="rect" id="node19" href="$_memory_manager_8c.html#a4dd1d910cde969a31ad009fcca1bb4a4" title="function used read/write and check the diving parameters in the memory. " alt="" coords="205,321,387,348"/>
<area shape="rect" id="node20" href="$_memory_manager_8c.html#a7161fed197cb374280e918eafb4d39a9" title="function used read/write and check the serial parameters in the memory. " alt="" coords="205,372,387,399"/>
<area shape="rect" id="node3" href="$_f_m25_v20_8c.html#a69f76e4332c185e885cdc6691bb075c2" title="FM25V20SetStatusReg" alt="" coords="453,132,611,159"/>
<area shape="rect" id="node6" href="$spi1_8c.html#afda94d01264dc64a8071f48ee19fb7c5" title="Function used to initialize the SPI1 module. " alt="" coords="499,56,565,83"/>
<area shape="rect" id="node4" href="$_f_m25_v20_8c.html#addeb196cb46ebc29e8f5e59e8dd01b15" title="Function used to set the write mode. " alt="" coords="661,157,837,184"/>
<area shape="rect" id="node5" href="$spi1_8c.html#a3d9bbade5a2bc2bfbc959fa5520cf3e0" title="Function used to send data over the SPI module 1. " alt="" coords="886,183,965,209"/>
<area shape="rect" id="node7" href="$_d_s_p__mkl16z256vlh4_8c.html#a2a50d72a0d050185db3317b26c26898f" title="SPI1ClockGate" alt="" coords="694,56,805,83"/>
<area shape="rect" id="node8" href="$_d_s_p__mkl16z256vlh4_8c.html#a632bf0f16c99bfa82c85594dea0d45df" title="SPI1PinMappingPeripheral" alt="" coords="661,5,837,32"/>
<area shape="rect" id="node10" href="$checksum_8c.html#aad26e4a22de65858452820ee23babd5a" title="Compute and return a checksum on the right data type. " alt="" coords="451,499,613,525"/>
<area shape="rect" id="node13" href="$_f_m25_v20_8c.html#adb5842f7204713f99fa6ce183317a523" title="Get the low power status of the memory. " alt="" coords="453,271,611,297"/>
<area shape="rect" id="node14" href="$_f_m25_v20_8c.html#ab71cea0f2db62d709c9b1a6441a70581" title="Put the memory in a low power mode. " alt="" coords="479,321,585,348"/>
<area shape="rect" id="node15" href="$_f_m25_v20_8c.html#ace631f94926ad79e89fdfd13013659e6" title="Read data from the memory. " alt="" coords="465,220,599,247"/>
<area shape="rect" id="node17" href="$_f_m25_v20_8c.html#a3866b69abe44cb40d09f89c2cc3ba8b3" title="Wake up the memory from the low power mode. " alt="" coords="468,372,596,399"/>
<area shape="rect" id="node16" href="$spi1_8c.html#a93ecc3b36648270cd041dad2bd467745" title="Function used to read data over the SPI module 1. " alt="" coords="710,283,789,309"/>
</map>
