<map id="Spi1Send" name="Spi1Send">
<area shape="rect" id="node2" href="$_f_m25_v20_8h.html#addeb196cb46ebc29e8f5e59e8dd01b15" title="Function used to set the write mode. " alt="" coords="133,436,309,463"/>
<area shape="rect" id="node3" href="$_f_m25_v20_8h.html#a69f76e4332c185e885cdc6691bb075c2" title="Functions used to set and read the status register. " alt="" coords="358,512,517,539"/>
<area shape="rect" id="node8" href="$_f_m25_v20_8h.html#a614bc8a001d6845b564f529dc542410d" title="Write data to the memory. " alt="" coords="369,316,505,343"/>
<area shape="rect" id="node25" href="$_f_m25_v20_8h.html#ab71cea0f2db62d709c9b1a6441a70581" title="Put the memory in a low power mode. " alt="" coords="385,461,490,488"/>
<area shape="rect" id="node32" href="$_f_m25_v20_8h.html#ace631f94926ad79e89fdfd13013659e6" title="Read data from the memory. " alt="" coords="370,259,505,285"/>
<area shape="rect" id="node33" href="$_f_m25_v20_8h.html#a81989bd9510f8ae046048c184c04feb2" title="Function used to read the device ID. " alt="" coords="143,537,299,564"/>
<area shape="rect" id="node34" href="$_f_m25_v20_8h.html#a35cd894c50c66a2bc5ebd81ab26bcfcf" title="Functions used to set and read the status register. " alt="" coords="137,588,306,615"/>
<area shape="rect" id="node4" href="$_f_m25_v20_8h.html#a2e18e393748dca1da43e4e069bc4972f" title="Function used to initialize the FM25V20 memory. " alt="" coords="630,765,725,792"/>
<area shape="rect" id="node5" href="$_memory_manager_8h.html#a75f5428e07dbdaee7b7d024a3447da8b" title="function use to initialize the memory manager. " alt="" coords="853,411,989,437"/>
<area shape="rect" id="node6" href="$main_8c.html#aadf3292d1b050137201649db87e63aa5" title="Function used to initialize all non critical peripheral. " alt="" coords="1324,479,1380,505"/>
<area shape="rect" id="node7" href="$main_8c.html#a6288eba0f8e8ad3ab1544ad731eb7667" title="Main function. " alt="" coords="1459,543,1509,569"/>
<area shape="rect" id="node9" href="$_f_m25_v20_mem_test_8h.html#a31b1c7bd95f8fc629c82fedbc7e86c19" title="FM25V20MemTest_Clear" alt="" coords="593,208,762,235"/>
<area shape="rect" id="node11" href="$_f_m25_v20_mem_test_8h.html#a5324c46da6daa18c72d434ddd2695b87" title="FM25V20MemTest_HighFreqDown" alt="" coords="566,259,789,285"/>
<area shape="rect" id="node12" href="$_f_m25_v20_mem_test_8h.html#a3dab3a8f4d5b585ffc341132a8905a4e" title="FM25V20MemTest_HighFreqUp" alt="" coords="574,5,781,32"/>
<area shape="rect" id="node13" href="$_f_m25_v20_mem_test_8h.html#aa801df1c3fb82c4b63ea3da6209ac73d" title="FM25V20MemTest_PulseN" alt="" coords="587,56,768,83"/>
<area shape="rect" id="node14" href="$_f_m25_v20_mem_test_8h.html#a5a0a75083ba30546c433ecb0b12edf3d" title="FM25V20MemTest_PulseP" alt="" coords="587,107,768,133"/>
<area shape="rect" id="node15" href="$_f_m25_v20_mem_test_8h.html#a4fa08b2f438caece8e0907091a74496f" title="FM25V20MemTest_Set" alt="" coords="598,157,757,184"/>
<area shape="rect" id="node16" href="$_memory_manager_8h.html#aa72a3e9863e2ac9b476266b1fad21575" title="function used read/write and check the log in the memory. " alt="" coords="592,512,763,539"/>
<area shape="rect" id="node20" href="$_memory_manager_8h.html#afff43e62869a6852a9b8e7c5c8683e25" title="function used read/write and check the diving parameters in the memory. " alt="" coords="585,563,769,589"/>
<area shape="rect" id="node21" href="$_memory_manager_8h.html#aaf68fcb13458866a83fe16fa9c66aca9" title="function used read/write and check the log in the memory. " alt="" coords="592,664,763,691"/>
<area shape="rect" id="node24" href="$_memory_manager_8h.html#a45e7b71d057b396d37a5867806284b40" title="function used read/write and check the serial parameters in the memory. " alt="" coords="586,613,769,640"/>
<area shape="rect" id="node10" href="$_f_m25_v20_mem_test_8h.html#a1294aa9668bfe5b70480e64ab33d5a20" title="FM25V20MemTest_Main" alt="" coords="838,132,1005,159"/>
<area shape="rect" id="node17" href="$_usb_manager_8h.html#ac8d1502564dd3480fc417f834a13cec2" title="Function use to deal received command. " alt="" coords="842,563,1001,589"/>
<area shape="rect" id="node18" href="$_usb_manager_8h.html#a1e480179c92fe988f89777f353e9ef9a" title="USB manager. " alt="" coords="1102,567,1197,593"/>
<area shape="rect" id="node19" href="$main_8c.html#a47b19cb17359b8a4930e1db6207395fb" title="Function used to deal background task. " alt="" coords="1294,605,1410,632"/>
<area shape="rect" id="node22" href="$_button_manager_8c.html#afdd019b240e44a51aba9069b09cd3ee8" title="ButtonManagerDealer" alt="" coords="848,652,995,679"/>
<area shape="rect" id="node23" href="$_button_manager_8h.html#a6131a6127b6045f5c352ca091ebdb36a" title="Button manager function. " alt="" coords="1094,643,1205,669"/>
<area shape="rect" id="node26" href="$_memory_manager_8h.html#a95c0f9ae110105c19fb6eb0da09930e0" title="Return the number of log stored in memory. " alt="" coords="571,309,783,336"/>
<area shape="rect" id="node27" href="$_memory_manager_8h.html#a4dd1d910cde969a31ad009fcca1bb4a4" title="function used read/write and check the diving parameters in the memory. " alt="" coords="586,360,769,387"/>
<area shape="rect" id="node28" href="$_memory_manager_8h.html#a4621c0be0193d08ee84b8dc8bdaea778" title="function used read/write and check the log in the memory. " alt="" coords="592,461,763,488"/>
<area shape="rect" id="node29" href="$_memory_manager_8h.html#a7161fed197cb374280e918eafb4d39a9" title="function used read/write and check the serial parameters in the memory. " alt="" coords="586,411,769,437"/>
<area shape="rect" id="node30" href="$_power_manager_8h.html#a7406ccf39ad8768c5043ac74da94a63b" title="Functions used to Enter and exit low power mode. " alt="" coords="594,715,761,741"/>
<area shape="rect" id="node31" href="$_power_manager_8h.html#aef7050cf231cfdbbdb4134de79e10add" title="Low Power mode controller. " alt="" coords="1054,705,1245,732"/>
</map>
