<map id="RFIDManager" name="RFIDManager">
<area shape="rect" id="node2" href="$_c_r95_uart_mapper_8c.html#a7ad185503043b02e75769ae9ebb3e6b9" title="Return the connection state of the CR95HF module. " alt="" coords="1053,461,1243,488"/>
<area shape="rect" id="node3" href="$_c_r95_h_f_8c.html#ac51f39d982f31bb7548abf2bd31065b5" title="Global manager of the CR95HF module. " alt="" coords="155,929,277,956"/>
<area shape="rect" id="node27" href="$tick_8c.html#a0145cffb9b0238336157774cbdb484a9" title="Get the milliseconds counter. " alt="" coords="1063,715,1233,741"/>
<area shape="rect" id="node28" href="$_r_f_i_d_manager_8c.html#ac7dc07d3fd12132286ea2fa1a90057b5" title="RFIDDealer" alt="" coords="619,411,707,437"/>
<area shape="rect" id="node4" href="$_c_r95_h_f_8c.html#a7698cb3b03ed1c1b43f76c3bb7f09ff7" title="CR95HFBufCompare" alt="" coords="345,980,487,1007"/>
<area shape="rect" id="node5" href="$_c_r95_h_f_8c.html#ad4ff927727333b1b7d9d241553e16cf0" title="CR95HFCommandManager" alt="" coords="326,929,506,956"/>
<area shape="rect" id="node22" href="$_c_r95_h_f_8c.html#a1bb7609ee8731724346fe17b790ebe84" title="CR95HFReadAnswer" alt="" coords="344,1157,488,1184"/>
<area shape="rect" id="node6" href="$_c_r95_h_f_8c.html#a01394d4b8512e2b08b85e45a77202f40" title="CR95HFBridgeStateMachine" alt="" coords="569,1056,757,1083"/>
<area shape="rect" id="node16" href="$_c_r95_h_f_8c.html#a736908fe7ee9f6d89001e672da4ddf63" title="CR95HFEchoStateMachine" alt="" coords="572,1107,753,1133"/>
<area shape="rect" id="node17" href="$_c_r95_h_f_8c.html#ad844ac3aea8ad245c43aad4f45878ef4" title="CR95HFField15693StateMachine" alt="" coords="555,853,770,880"/>
<area shape="rect" id="node18" href="$_c_r95_h_f_8c.html#a3b757ae22ec0926378098fa5bc16a51b" title="CR95HFFieldOffStateMachine" alt="" coords="565,904,760,931"/>
<area shape="rect" id="node19" href="$_c_r95_h_f_8c.html#a33750c8ee6d29c851f990d2eda5f0e45" title="CR95HFHibernateStateMachine" alt="" coords="559,803,766,829"/>
<area shape="rect" id="node20" href="$_c_r95_h_f_8c.html#a5e26b7bcad0e2958c3a0bd78fbdf9198" title="CR95HFReadStateMachine" alt="" coords="572,955,753,981"/>
<area shape="rect" id="node21" href="$_c_r95_h_f_8c.html#ade2c9e959b711283ff94bab4ba81032b" title="CR95HFWriteStateMachine" alt="" coords="571,1005,754,1032"/>
<area shape="rect" id="node7" href="$_c_r95_h_f_8c.html#a97649b66ce11fc9fe4f934ada503cdbd" title="CR95HFWriteCommand" alt="" coords="826,968,987,995"/>
<area shape="rect" id="node8" href="$_c_r95_uart_mapper_8c.html#a073808c89f3a15ef8044992f7ec9ccdb" title="CR95UartDisableReceiver" alt="" coords="1063,816,1233,843"/>
<area shape="rect" id="node9" href="$_c_r95_uart_mapper_8c.html#ae83438c457cf2e15ca86ef6f1993ca66" title="CR95UartEnableReceiver" alt="" coords="1065,968,1231,995"/>
<area shape="rect" id="node10" href="$_c_r95_uart_mapper_8c.html#aa9dd826de5b784fbd0569e6d12be8397" title="Reset the CR95HF Uart interface. " alt="" coords="1067,1019,1229,1045"/>
<area shape="rect" id="node11" href="$_c_r95_uart_mapper_8c.html#aa48280ff1cfa4743c04d90e8b18c7144" title="CR95UartSendData" alt="" coords="1081,563,1215,589"/>
<area shape="rect" id="node14" href="$_string_tools_8c.html#a686b87edf1f7ea01913b46650244206c" title="Clear a string (reset all char to &#39;\0&#39;). " alt="" coords="1081,1120,1215,1147"/>
<area shape="rect" id="node15" href="$tick_8c.html#aa43bd4bc67b26f7e7ab31be06b088a14" title="Get the milliseconds counter. " alt="" coords="1301,715,1432,741"/>
<area shape="rect" id="node12" href="$uart0_8c.html#a702d354b2f7a798728f7b564c6a5bc35" title="send data other uart. " alt="" coords="1311,588,1422,615"/>
<area shape="rect" id="node13" href="$uart2_8c.html#abc17789ee9265fd32a53f68b0c16d2d8" title="send data other uart. " alt="" coords="1311,537,1422,564"/>
<area shape="rect" id="node23" href="$_c_r95_uart_mapper_8c.html#aacdf1bb5e1f6d3efca030a260dce0111" title="Return the structure control of the CR95HF uart. " alt="" coords="573,1208,752,1235"/>
<area shape="rect" id="node24" href="$_c_r95_uart_mapper_8c.html#ad29a6e98583a389413f39cfddacdd5c6" title="CR95UartReadChar" alt="" coords="595,1157,730,1184"/>
<area shape="rect" id="node25" href="$uart0_8c.html#a707377413c7c1f2c9c884af517f9dedc" title="Uart0ReadChar" alt="" coords="851,1132,962,1159"/>
<area shape="rect" id="node26" href="$uart2_8c.html#a7134deb099ba4ba321fe2f41b398b37e" title="Uart2ReadChar" alt="" coords="851,1183,962,1209"/>
<area shape="rect" id="node29" href="$_r_f_i_d_manager_8c.html#a6ab6b8dd0e473d8fdf4a01c3ffbd7852" title="RFIDBridgeStateMachine" alt="" coords="823,411,991,437"/>
<area shape="rect" id="node37" href="$_r_f_i_d_manager_8c.html#aaadf0da29bf3176eb69c6e8ec6e08a6b" title="RFIDExtLpmStateMachine" alt="" coords="819,259,995,285"/>
<area shape="rect" id="node40" href="$_r_f_i_d_manager_8c.html#a76aaad614e4215dd0b1f0a55c91448ff" title="RFIDIntLpmStateMachine" alt="" coords="821,309,992,336"/>
<area shape="rect" id="node41" href="$_r_f_i_d_manager_8c.html#a776bd19e29a44fe5b562330efe4b1808" title="RFIDReadStateMachine" alt="" coords="826,512,987,539"/>
<area shape="rect" id="node43" href="$_r_f_i_d_manager_8c.html#aa800930fc21149f77f2b93ece7ede47b" title="RFIDWriteStateMachine" alt="" coords="825,563,988,589"/>
<area shape="rect" id="node30" href="$_c_r95_h_f_8c.html#a652e787d25427bedbd66533629298f5a" title="Return the current state of the CR95HF module in it&#39;s manager. " alt="" coords="1064,259,1232,285"/>
<area shape="rect" id="node31" href="$_c_r95_h_f_8c.html#ab73c2e7ae98f669c93c235a762f27649" title="CR95HFStartBridge" alt="" coords="1080,107,1216,133"/>
<area shape="rect" id="node32" href="$_c_r95_h_f_8c.html#af52d793b7c0dbefdfa0b2060f0366a3d" title="Manager used to deal each specific state. " alt="" coords="1083,309,1213,336"/>
<area shape="rect" id="node33" href="$_c_r95_h_f_8c.html#a27506223088d2179f105cc721bd17d99" title="CR95HFStartField15693" alt="" coords="1067,512,1229,539"/>
<area shape="rect" id="node34" href="$_c_r95_uart_mapper_8c.html#ae9b7dcc01097b34d264ecc59cfd3659e" title="Select the antenna used to communicate with the SRD. " alt="" coords="1083,360,1213,387"/>
<area shape="rect" id="node35" href="$_usb_manager_8c.html#a3faf19ddc73b0a9e25c5b66dd5b49bff" title="Function used to send the CR95 error on the USB. " alt="" coords="1055,157,1241,184"/>
<area shape="rect" id="node36" href="$_usb_manager_8c.html#a9246dcc92e2a78422be0a94688fcf853" title="Function used to send the CR95 result of last RFID operation on the USB. " alt="" coords="1051,208,1245,235"/>
<area shape="rect" id="node38" href="$_c_r95_h_f_8c.html#a1291f99a43efc55ba45a58ffb5899c8e" title="CR95HFStartFieldOff" alt="" coords="1077,56,1219,83"/>
<area shape="rect" id="node39" href="$_c_r95_h_f_8c.html#a35fb88e6119a4cfa8f0014973f6339ce" title="CR95HFStartHibernate" alt="" coords="1071,5,1225,32"/>
<area shape="rect" id="node42" href="$_c_r95_h_f_8c.html#ae8388513b3c386e588c3539aded54006" title="CR95HFStartRead" alt="" coords="1083,664,1213,691"/>
<area shape="rect" id="node44" href="$_c_r95_h_f_8c.html#aba2c35a53fa89e7805a8513d98981a69" title="CR95HFStartWrite" alt="" coords="1083,867,1213,893"/>
<area shape="rect" id="node45" href="$checksum_8c.html#aea3900f8f3c22134b50fbb7fe78a487b" title="ChecksumByteOnShortCompute" alt="" coords="1043,917,1253,944"/>
</map>
