<map id="CriticalInit" name="CriticalInit">
<area shape="rect" id="node2" href="$device_8c.html#a631a644dd7e158b7fa45c4bfe43b29bc" title="Function to switch the processor on the highest clock speed allowed. " alt="" coords="133,5,328,32"/>
<area shape="rect" id="node3" href="$device_8c.html#a9237af6f7adfd2b81439ae8542694b8b" title="Function to initialize the device clock. " alt="" coords="192,56,269,83"/>
<area shape="rect" id="node5" href="$rtc_8c.html#aa884644b359833678d1f4bde7c214e32" title="Function used to initialized the RTC module. " alt="" coords="201,107,260,133"/>
<area shape="rect" id="node6" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="177,157,284,184"/>
<area shape="rect" id="node7" href="$watchdog_8c.html#a4f58d14b66f9b050c560664b217964d7" title="start watchdog (can be call only ones and can&#39;t call after WatchdogStop()). " alt="" coords="176,208,285,235"/>
<area shape="rect" id="node4" href="$device_8c.html#af0b6ea9b67bd97df7598273a732fedeb" title="Function to switch the processor clock on the FEI clock source. " alt="" coords="376,56,568,83"/>
</map>
