<map id="PowerManager" name="PowerManager">
<area shape="rect" id="node2" href="$_b_q27510_d_r_z_r_g2_8c.html#ab6764798c058c46b3cdcf21c97027ffb" title="Function used to get all information about the cell monitoring. " alt="" coords="208,459,315,486"/>
<area shape="rect" id="node23" href="$_power_manager_8c.html#a851ecff0a5e93c3b261accadbf32621b" title="PowerManagerDisplayLoaded" alt="" coords="165,915,358,942"/>
<area shape="rect" id="node31" href="$_power_manager_8c.html#aa781287c32b2238935eb53a6ce806419" title="PowerManagerDisplayLoading" alt="" coords="163,966,359,992"/>
<area shape="rect" id="node34" href="$_power_manager_8c.html#a20ccb5a44ea9c3ecb98d6ec3ed84c62a" title="PowerManagerDisplayLoading\lError" alt="" coords="163,1017,359,1058"/>
<area shape="rect" id="node3" href="$_b_q27510_d_r_z_r_g2_8c.html#ab9dcad56c77f04971532555567a0d84b" title="Function used to know if a battery is connected or not. " alt="" coords="680,180,840,207"/>
<area shape="rect" id="node5" href="$_b_q27510_d_r_z_r_g2_8c.html#ac5d4fef49e298779b1753f40cf601cd3" title="BQ_getAvailableEnergy" alt="" coords="437,256,595,283"/>
<area shape="rect" id="node7" href="$_b_q27510_d_r_z_r_g2_8c.html#a9854bebed505691984f1cfa674cb3cb1" title="BQ_getAverageCurrent" alt="" coords="439,307,593,334"/>
<area shape="rect" id="node8" href="$_b_q27510_d_r_z_r_g2_8c.html#a28acfc3f3d1ff8e9d9d91edadc29ecd5" title="BQ_getAveragePower" alt="" coords="442,358,590,384"/>
<area shape="rect" id="node9" href="$_b_q27510_d_r_z_r_g2_8c.html#af8268e396eeb7abdfb21a7fbf03f1396" title="Function used to get some information about the cell monitoring. " alt="" coords="436,408,596,435"/>
<area shape="rect" id="node10" href="$_b_q27510_d_r_z_r_g2_8c.html#af6d8cc1ca065bcb90798788851de572c" title="BQ_getCellVoltage" alt="" coords="450,459,582,486"/>
<area shape="rect" id="node11" href="$_b_q27510_d_r_z_r_g2_8c.html#a02b013ae0aec405f9c7ceb909199f5f0" title="BQ_getCycleCount" alt="" coords="449,510,583,536"/>
<area shape="rect" id="node12" href="$_b_q27510_d_r_z_r_g2_8c.html#aaead900b00cb48e635c7db154f99c3e5" title="BQ_getFullAvailableCapacity" alt="" coords="421,560,611,587"/>
<area shape="rect" id="node13" href="$_b_q27510_d_r_z_r_g2_8c.html#a148f18dc993b083cacc31ff1f4dc71ed" title="BQ_getFullChargeCapacity" alt="" coords="427,611,605,638"/>
<area shape="rect" id="node14" href="$_b_q27510_d_r_z_r_g2_8c.html#a42dac1127d0914053de05fd9af45b77a" title="BQ_getMaxLoadCurrent" alt="" coords="435,662,597,688"/>
<area shape="rect" id="node15" href="$_b_q27510_d_r_z_r_g2_8c.html#aa723c8cc7b39b74ae4c344cb39350aed" title="BQ_getMaxLoadTimeToEmpty" alt="" coords="417,712,615,739"/>
<area shape="rect" id="node16" href="$_b_q27510_d_r_z_r_g2_8c.html#a14b533c028c320fc9b2a5b9043d0e259" title="BQ_getNominalAvailableCapacity" alt="" coords="409,763,623,790"/>
<area shape="rect" id="node17" href="$_b_q27510_d_r_z_r_g2_8c.html#a6602062ce84e9142bfab316784516eb8" title="BQ_getRemainingCapacity" alt="" coords="427,814,605,840"/>
<area shape="rect" id="node18" href="$_b_q27510_d_r_z_r_g2_8c.html#a3a21f0765f44c716b638d8b8773946d2" title="BQ_getStandbyTimeToEmpty" alt="" coords="419,864,613,891"/>
<area shape="rect" id="node19" href="$_b_q27510_d_r_z_r_g2_8c.html#a84d862a65a34dff063b11338b89a5931" title="BQ_getStateOfCharge" alt="" coords="441,54,591,80"/>
<area shape="rect" id="node20" href="$_b_q27510_d_r_z_r_g2_8c.html#ab0c39d16ad675e6a83e2659c9a51551b" title="BQ_getTimeToEmpty" alt="" coords="443,104,589,131"/>
<area shape="rect" id="node21" href="$_b_q27510_d_r_z_r_g2_8c.html#aade4e442c60a3cf1aa9223a7696483dc" title="BQ_getTimeToFull" alt="" coords="451,155,581,182"/>
<area shape="rect" id="node22" href="$_b_q27510_d_r_z_r_g2_8c.html#a8a62d091a91f6665acc0bd38ee9af9da" title="BQ_getTTEAtConstantPower" alt="" coords="421,206,611,232"/>
<area shape="rect" id="node4" href="$i2c0_8c.html#ada7d730a8793a6ddd23180047b309447" title="Send a packet on the I2C interface. " alt="" coords="897,307,975,334"/>
<area shape="rect" id="node6" href="$i2c0_8c.html#a1f3862c3506c31b0a50c7914f17314ab" title="Read a packet on the I2C interface. " alt="" coords="721,434,799,460"/>
<area shape="rect" id="node24" href="$display_8c.html#ad8f9098d6f81dbce9ff70ef99662f212" title="Function used get the data displayed. " alt="" coords="431,915,601,942"/>
<area shape="rect" id="node25" href="$display_8c.html#a0529c896e4069df4bb7c4e767f36be28" title="Function used set the data displayed. " alt="" coords="431,966,601,992"/>
<area shape="rect" id="node26" href="$decoder16_seg_8c.html#a2d2fc41a03a66256e4681e8d695f01b0" title="Function used to decode a char and display it on a 16 segments digit. " alt="" coords="680,1054,840,1080"/>
<area shape="rect" id="node27" href="$decoder7_seg_8c.html#a8e8cab35cf7c9517f7094f42637a086e" title="Function used to decode a char and display it on a 7 segments digit. " alt="" coords="683,827,837,854"/>
<area shape="rect" id="node28" href="$display_8c.html#a771439bf50110fb999649ac3262bc4ef" title="Function used to root 16 segments command on the rigth PIN. " alt="" coords="689,878,831,904"/>
<area shape="rect" id="node29" href="$display_8c.html#ace411722dfe7b549d16c09991a5ff24f" title="Function used to root 7 segments command on the rigth PIN. " alt="" coords="693,928,827,955"/>
<area shape="rect" id="node30" href="$spi0_8c.html#a6d528a26e3df5e8bdb80622df3946998" title="Function used to send data over the SPI module 0. " alt="" coords="721,1003,799,1030"/>
<area shape="rect" id="node32" href="$display_8c.html#a20d8e5860540ecfe3c0bb5a237bc17f8" title="Function used to enable/disable the display power. " alt="" coords="455,1024,577,1051"/>
<area shape="rect" id="node33" href="$_d_s_p__mkl16z256vlh4_8c.html#ad30b60ccfc1302cb250629c495851333" title="Functions to MAP the defined IO of the SPI module x in the rigth pin. " alt="" coords="672,1104,848,1131"/>
</map>
