<map id="RFIDBridgeStateMachine" name="RFIDBridgeStateMachine">
<area shape="rect" id="node2" href="$_c_r95_uart_mapper_8c.html#a7ad185503043b02e75769ae9ebb3e6b9" title="Return the connection state of the CR95HF module. " alt="" coords="223,5,414,32"/>
<area shape="rect" id="node3" href="$_c_r95_h_f_8c.html#a652e787d25427bedbd66533629298f5a" title="Return the current state of the CR95HF module in it&#39;s manager. " alt="" coords="235,56,403,83"/>
<area shape="rect" id="node4" href="$_c_r95_h_f_8c.html#ab73c2e7ae98f669c93c235a762f27649" title="CR95HFStartBridge" alt="" coords="251,107,387,133"/>
<area shape="rect" id="node5" href="$_c_r95_h_f_8c.html#af52d793b7c0dbefdfa0b2060f0366a3d" title="Manager used to deal each specific state. " alt="" coords="254,157,383,184"/>
<area shape="rect" id="node6" href="$_c_r95_h_f_8c.html#a27506223088d2179f105cc721bd17d99" title="CR95HFStartField15693" alt="" coords="237,208,400,235"/>
<area shape="rect" id="node7" href="$_c_r95_uart_mapper_8c.html#ae9b7dcc01097b34d264ecc59cfd3659e" title="Select the antenna used to communicate with the SRD. " alt="" coords="254,259,383,285"/>
<area shape="rect" id="node8" href="$_c_r95_uart_mapper_8c.html#a073808c89f3a15ef8044992f7ec9ccdb" title="CR95UartDisableReceiver" alt="" coords="233,309,404,336"/>
<area shape="rect" id="node9" href="$_c_r95_uart_mapper_8c.html#aa48280ff1cfa4743c04d90e8b18c7144" title="CR95UartSendData" alt="" coords="251,360,386,387"/>
<area shape="rect" id="node12" href="$tick_8c.html#aa43bd4bc67b26f7e7ab31be06b088a14" title="Get the milliseconds counter. " alt="" coords="464,448,595,475"/>
<area shape="rect" id="node13" href="$tick_8c.html#a0145cffb9b0238336157774cbdb484a9" title="Get the milliseconds counter. " alt="" coords="234,461,403,488"/>
<area shape="rect" id="node14" href="$_usb_manager_8c.html#a3faf19ddc73b0a9e25c5b66dd5b49bff" title="Function used to send the CR95 error on the USB. " alt="" coords="226,512,411,539"/>
<area shape="rect" id="node15" href="$_usb_manager_8c.html#a9246dcc92e2a78422be0a94688fcf853" title="Function used to send the CR95 result of last RFID operation on the USB. " alt="" coords="221,563,416,589"/>
<area shape="rect" id="node10" href="$uart0_8c.html#a702d354b2f7a798728f7b564c6a5bc35" title="send data other uart. " alt="" coords="474,335,585,361"/>
<area shape="rect" id="node11" href="$uart2_8c.html#abc17789ee9265fd32a53f68b0c16d2d8" title="send data other uart. " alt="" coords="474,385,585,412"/>
</map>
