SRD Standelone programmation box: Globals

| SRD Standelone programmation box 2.0 (16/11/15 10:00:00) Documentation of the SRD standelone programmation box

- Main Page
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Enumerations
- Enumerator
- Macros

- b
- c
- d
- f
- g
- h
- i
- l
- m
- n
- p
- r
- s
- t
- u
- w
- x

All Data Structures Files Functions Variables Enumerations Enumerator Macros Pages
Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - c -

- ChecksumByteCompute() : checksum.c , checksum.h
- ChecksumByteOnShortCompute() : checksum.h , checksum.c
- ChecksumLongCompute() : checksum.c , checksum.h
- ChecksumShortCompute() : checksum.h , checksum.c
- CR95_EXT_CONNECTED : CR95UartMapper.h
- CR95_EXT_UNCONNECTED : CR95UartMapper.h
- CR95_SELECT_EXTERNAL : CR95UartMapper.h
- CR95_SELECT_INTERNAL : CR95UartMapper.h
- CR95DeviceSelected : CR95UartMapper.c
- CR95ExtGetConnectionState() : CR95UartMapper.c , CR95UartMapper.h
- CR95HF_ANSWER_BUF_SIZE : CR95HF.h
- CR95HF_BridgeState_Finish : CR95HF.h
- CR95HF_BridgeState_Send : CR95HF.h
- CR95HF_BridgeState_Start : CR95HF.h
- CR95HF_BridgeState_WaitAnswer : CR95HF.h
- CR95HF_COMMAND_BRIDGE : CR95HF.h
- CR95HF_COMMAND_ECHO : CR95HF.h
- CR95HF_COMMAND_FIELD15693 : CR95HF.h
- CR95HF_COMMAND_FIELDOFF : CR95HF.h
- CR95HF_COMMAND_HIBERNATE : CR95HF.h
- CR95HF_COMMAND_NONE : CR95HF.h
- CR95HF_COMMAND_READ : CR95HF.h
- CR95HF_COMMAND_WRITE : CR95HF.h
- CR95HF_ECHO_MAX_TRY : CR95HF.h
- CR95HF_EchoState_Finish : CR95HF.h
- CR95HF_EchoState_Send : CR95HF.h
- CR95HF_EchoState_Start : CR95HF.h
- CR95HF_EchoState_WaitAnswer : CR95HF.h
- CR95HF_Field15693State_Finish : CR95HF.h
- CR95HF_Field15693State_Send : CR95HF.h
- CR95HF_Field15693State_Start : CR95HF.h
- CR95HF_Field15693State_WaitAnswer : CR95HF.h
- CR95HF_FieldOffState_Finish : CR95HF.h
- CR95HF_FieldOffState_Send : CR95HF.h
- CR95HF_FieldOffState_Start : CR95HF.h
- CR95HF_FieldOffState_WaitAnswer : CR95HF.h
- CR95HF_FRAME_ANS_ECHO : CR95HF.c
- CR95HF_FRAME_ANS_ECHO_SIZE : CR95HF.c
- CR95HF_FRAME_CMD_ECHO : CR95HF.c
- CR95HF_FRAME_CMD_ECHO_SIZE : CR95HF.c
- CR95HF_HibernateState_Finish : CR95HF.h
- CR95HF_HibernateState_Send : CR95HF.h
- CR95HF_HibernateState_Start : CR95HF.h
- CR95HF_HibernateState_WaitAnswer : CR95HF.h
- CR95HF_IS_BUSY : CR95HF.h
- CR95HF_IS_READY : CR95HF.h
- CR95HF_ReadState_Finish : CR95HF.h
- CR95HF_ReadState_Send : CR95HF.h
- CR95HF_ReadState_Start : CR95HF.h
- CR95HF_ReadState_WaitAnswer : CR95HF.h
- CR95HF_RETURN_BUSY : CR95HF.h
- CR95HF_RETURN_ECHO_ERROR : CR95HF.h
- CR95HF_RETURN_FIELD15693_ERROR : CR95HF.h
- CR95HF_RETURN_FIELDOFF_ERROR : CR95HF.h
- CR95HF_RETURN_HIBERNATE_ERROR : CR95HF.h
- CR95HF_RETURN_OK : CR95HF.h
- CR95HF_RETURN_READ_ERROR : CR95HF.h
- CR95HF_RETURN_STATEMACHINE_ERROR : CR95HF.h
- CR95HF_RETURN_WORKING : CR95HF.h
- CR95HF_RETURN_WRITE_ERROR : CR95HF.h
- CR95HF_RX_BUF_SIZE : CR95HF.h
- CR95HF_UART_BAUDRATE : CR95HF.h
- CR95HF_WriteState_Finish : CR95HF.h
- CR95HF_WriteState_Send : CR95HF.h
- CR95HF_WriteState_Start : CR95HF.h
- CR95HF_WriteState_WaitAnswer : CR95HF.h
- CR95HFBridgeStateMachine() : CR95HF.c
- CR95HFBufCompare() : CR95HF.c
- CR95HFCommandManager() : CR95HF.c
- CR95HFCtrl : CR95HF.h , CR95HF.c
- CR95HFEchoStateMachine() : CR95HF.c
- CR95HFField15693StateMachine() : CR95HF.c
- CR95HFFieldOffStateMachine() : CR95HF.c
- CR95HFHibernateStateMachine() : CR95HF.c
- CR95HFInit() : CR95HF.c , CR95HF.h
- CR95HFManager() : CR95HF.c , CR95HF.h
- CR95HFManagerIsReady() : CR95HF.c , CR95HF.h
- CR95HFReadAnswer() : CR95HF.c
- CR95HFReadStateMachine() : CR95HF.c
- CR95HFStartBridge() : CR95HF.c , CR95HF.h
- CR95HFStartEcho() : CR95HF.c , CR95HF.h
- CR95HFStartField15693() : CR95HF.c , CR95HF.h
- CR95HFStartFieldOff() : CR95HF.h , CR95HF.c
- CR95HFStartHibernate() : CR95HF.h , CR95HF.c
- CR95HFStartRead() : CR95HF.h , CR95HF.c
- CR95HFStartWrite() : CR95HF.c , CR95HF.h
- CR95HFWriteCommand() : CR95HF.c
- CR95HFWriteStateMachine() : CR95HF.c
- CR95SelectDevice() : CR95UartMapper.h , CR95UartMapper.c
- CR95UartClearAllErrorFlag() : CR95UartMapper.h , CR95UartMapper.c
- CR95UartDisableReceiver() : CR95UartMapper.h , CR95UartMapper.c
- CR95UartDisableTransmitter() : CR95UartMapper.c , CR95UartMapper.h
- CR95UartEnableReceiver() : CR95UartMapper.h , CR95UartMapper.c
- CR95UartEnableTransmitter() : CR95UartMapper.c , CR95UartMapper.h
- CR95UartGetUartStructCtrl() : CR95UartMapper.c , CR95UartMapper.h
- CR95UartInit() : CR95UartMapper.c , CR95UartMapper.h
- CR95UARTMAPPER_EXTERNAL_CO_MASK : CR95UartMapper.h
- CR95UARTMAPPER_EXTERNAL_CO_SHIFT : CR95UartMapper.h
- CR95UartReadChar() : CR95UartMapper.h , CR95UartMapper.c
- CR95UartResetReceiver() : CR95UartMapper.h , CR95UartMapper.c
- CR95UartSendData() : CR95UartMapper.c , CR95UartMapper.h
- CR95UartSendString() : CR95UartMapper.c , CR95UartMapper.h
- CriticalInit() : main.c
- currentDigit : display.c