<map id="Setup" name="Setup">
<area shape="rect" id="node2" href="$_button_manager_8c.html#ae84a2c976c6278b78207e3ec6c6a2533" title="Function used to initialize the button manager. " alt="" coords="110,156,237,183"/>
<area shape="rect" id="node4" href="$display_8c.html#ae2c5b80a65268def4100ad7a1683b196" title="Function used to initialized the display. " alt="" coords="132,232,215,259"/>
<area shape="rect" id="node14" href="$display_8c.html#a20d8e5860540ecfe3c0bb5a237bc17f8" title="Function used to enable/disable the display power. " alt="" coords="113,460,234,487"/>
<area shape="rect" id="node15" href="$led_8c.html#a1d5b4eaf7f01ae9557ba620158ebdfd9" title="Function used to initialize the leds. " alt="" coords="143,561,203,588"/>
<area shape="rect" id="node16" href="$_memory_manager_8c.html#a75f5428e07dbdaee7b7d024a3447da8b" title="function use to initialize the memory manager. " alt="" coords="348,561,484,588"/>
<area shape="rect" id="node24" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="891,739,997,765"/>
<area shape="rect" id="node36" href="$_power_manager_8c.html#a6fc2f38d8cafdafb419605fddc230248" title="Variable used by the power manager. " alt="" coords="111,891,236,917"/>
<area shape="rect" id="node44" href="$_r_f_i_d_manager_8c.html#a67c55a98971bdbdc992fd3c60daebcc8" title="Function used to initialize the RFID manager. " alt="" coords="114,789,233,816"/>
<area shape="rect" id="node48" href="$tick_8c.html#a85de8acefef2c29ca44aa9728de87f92" title="Function used to initialize the Tick module . " alt="" coords="142,1043,205,1069"/>
<area shape="rect" id="node3" href="$button_8c.html#a30a1cff81be3c91e307685387401e863" title="Function used to initialized the buttons. " alt="" coords="377,131,455,157"/>
<area shape="rect" id="node5" href="$display_8c.html#a0529c896e4069df4bb7c4e767f36be28" title="Function used set the data displayed. " alt="" coords="331,232,501,259"/>
<area shape="rect" id="node11" href="$spi0_8c.html#aed55957fe67d7fa37fe71657a3a23885" title="Function used to initialize the SPI0 module. " alt="" coords="383,181,449,208"/>
<area shape="rect" id="node6" href="$decoder16_seg_8c.html#a2d2fc41a03a66256e4681e8d695f01b0" title="Function used to decode a char and display it on a 16 segments digit. " alt="" coords="621,232,781,259"/>
<area shape="rect" id="node7" href="$decoder7_seg_8c.html#a8e8cab35cf7c9517f7094f42637a086e" title="Function used to decode a char and display it on a 7 segments digit. " alt="" coords="625,283,778,309"/>
<area shape="rect" id="node8" href="$display_8c.html#a771439bf50110fb999649ac3262bc4ef" title="Function used to root 16 segments command on the rigth PIN. " alt="" coords="630,56,773,83"/>
<area shape="rect" id="node9" href="$display_8c.html#ace411722dfe7b549d16c09991a5ff24f" title="Function used to root 7 segments command on the rigth PIN. " alt="" coords="634,107,769,133"/>
<area shape="rect" id="node10" href="$spi0_8c.html#a6d528a26e3df5e8bdb80622df3946998" title="Function used to send data over the SPI module 0. " alt="" coords="662,181,741,208"/>
<area shape="rect" id="node12" href="$_d_s_p__mkl16z256vlh4_8c.html#a8cb70b7bf7cf14483f458de503ff6f6b" title="Functions to enable/disable the main clock of the specified SPI. " alt="" coords="646,5,757,32"/>
<area shape="rect" id="node13" href="$_d_s_p__mkl16z256vlh4_8c.html#ad30b60ccfc1302cb250629c495851333" title="Functions to MAP the defined IO of the SPI module x in the rigth pin. " alt="" coords="613,333,789,360"/>
<area shape="rect" id="node17" href="$_f_m25_v20_8c.html#a2e18e393748dca1da43e4e069bc4972f" title="Function used to initialize the FM25V20 memory. " alt="" coords="654,485,749,512"/>
<area shape="rect" id="node25" href="$_memory_manager_8c.html#a4dd1d910cde969a31ad009fcca1bb4a4" title="function used read/write and check the diving parameters in the memory. " alt="" coords="610,587,793,613"/>
<area shape="rect" id="node31" href="$_memory_manager_8c.html#a23afd9881c251d81c7ff88b4fefbb8e4" title="MemoryManagerCheckDiving" alt="" coords="606,384,797,411"/>
<area shape="rect" id="node33" href="$_memory_manager_8c.html#a7161fed197cb374280e918eafb4d39a9" title="function used read/write and check the serial parameters in the memory. " alt="" coords="610,637,793,664"/>
<area shape="rect" id="node34" href="$_memory_manager_8c.html#a7b3973e4132860fb79b75c73bc111a6f" title="MemoryManagerCheckSerial" alt="" coords="607,435,796,461"/>
<area shape="rect" id="node35" href="$_memory_manager_8c.html#a95c0f9ae110105c19fb6eb0da09930e0" title="Return the number of log stored in memory. " alt="" coords="595,536,807,563"/>
<area shape="rect" id="node18" href="$_f_m25_v20_8c.html#a69f76e4332c185e885cdc6691bb075c2" title="FM25V20SetStatusReg" alt="" coords="865,435,1023,461"/>
<area shape="rect" id="node21" href="$spi1_8c.html#afda94d01264dc64a8071f48ee19fb7c5" title="Function used to initialize the SPI1 module. " alt="" coords="911,485,977,512"/>
<area shape="rect" id="node19" href="$_f_m25_v20_8c.html#addeb196cb46ebc29e8f5e59e8dd01b15" title="Function used to set the write mode. " alt="" coords="1080,384,1256,411"/>
<area shape="rect" id="node20" href="$spi1_8c.html#a3d9bbade5a2bc2bfbc959fa5520cf3e0" title="Function used to send data over the SPI module 1. " alt="" coords="1305,511,1383,537"/>
<area shape="rect" id="node22" href="$_d_s_p__mkl16z256vlh4_8c.html#a2a50d72a0d050185db3317b26c26898f" title="SPI1ClockGate" alt="" coords="1113,485,1223,512"/>
<area shape="rect" id="node23" href="$_d_s_p__mkl16z256vlh4_8c.html#a632bf0f16c99bfa82c85594dea0d45df" title="SPI1PinMappingPeripheral" alt="" coords="1080,536,1256,563"/>
<area shape="rect" id="node26" href="$_f_m25_v20_8c.html#adb5842f7204713f99fa6ce183317a523" title="Get the low power status of the memory. " alt="" coords="865,688,1023,715"/>
<area shape="rect" id="node27" href="$_f_m25_v20_8c.html#a3866b69abe44cb40d09f89c2cc3ba8b3" title="Wake up the memory from the low power mode. " alt="" coords="880,536,1008,563"/>
<area shape="rect" id="node28" href="$_f_m25_v20_8c.html#ace631f94926ad79e89fdfd13013659e6" title="Read data from the memory. " alt="" coords="877,587,1011,613"/>
<area shape="rect" id="node30" href="$_f_m25_v20_8c.html#ab71cea0f2db62d709c9b1a6441a70581" title="Put the memory in a low power mode. " alt="" coords="891,637,997,664"/>
<area shape="rect" id="node29" href="$spi1_8c.html#a93ecc3b36648270cd041dad2bd467745" title="Function used to read data over the SPI module 1. " alt="" coords="1129,661,1207,688"/>
<area shape="rect" id="node32" href="$checksum_8c.html#aad26e4a22de65858452820ee23babd5a" title="Compute and return a checksum on the right data type. " alt="" coords="863,384,1025,411"/>
<area shape="rect" id="node37" href="$_l_t_c4160_8c.html#a6314c6a65847fe9ede22c7c54dee4029" title="Initialize the LTC4160 device. " alt="" coords="371,992,461,1019"/>
<area shape="rect" id="node38" href="$_b_q27510_d_r_z_r_g2_8c.html#a2cb45043dac162bf292c5613f6f9fe68" title="Function used to initialize the BQ device and it&#39;s DSP peripheral. " alt="" coords="341,840,491,867"/>
<area shape="rect" id="node42" href="$_l_t_c4160_8c.html#a1859ad97d50351b41fa4ddad7ad928c8" title="Define the current limit drawn by the charger. " alt="" coords="354,891,478,917"/>
<area shape="rect" id="node43" href="$_power_manager_8c.html#ad82283ab9a30920f56833e7d42dd66c8" title="PowerManagerClearWakeUpInterruptFlag" alt="" coords="286,941,546,968"/>
<area shape="rect" id="node39" href="$i2c0_8c.html#afb1f62a78531bcfd5f2081d1b64e43ad" title="Initialized the I2C0 module with the defined parameters. " alt="" coords="669,840,734,867"/>
<area shape="rect" id="node40" href="$_d_s_p__mkl16z256vlh4_8c.html#a5e21c411f7c8bdda9dc52bb6114ab9f4" title="Functions to enable/disable the main clock of the specified I2C. " alt="" coords="889,891,999,917"/>
<area shape="rect" id="node41" href="$_d_s_p__mkl16z256vlh4_8c.html#a5f699c7ddbcad4b8d84fa41305dfec3f" title="Functions to MAP the defined IO of the I2C module x in the rigth pin. " alt="" coords="857,840,1031,867"/>
<area shape="rect" id="node45" href="$_c_r95_h_f_8c.html#a5a280da3bb75613fbb5e62854ec65e3a" title="Function used to initialize the CR95HF global manager. " alt="" coords="372,789,460,816"/>
<area shape="rect" id="node46" href="$_c_r95_uart_mapper_8c.html#a530fdd7929335f4103bf44a111d9f441" title="CR95HF Uart interface. " alt="" coords="654,789,749,816"/>
<area shape="rect" id="node47" href="$uart0_8c.html#a2ed82ee365da2b37ca2446c607b38a4e" title="Initialize this uart. " alt="" coords="909,789,979,816"/>
<area shape="rect" id="node49" href="$pit_8c.html#a77b58f0272b0bdf0cc4d7705b4627c77" title="Initialize a PIT module. " alt="" coords="389,1093,443,1120"/>
<area shape="rect" id="node50" href="$tick_8c.html#a0e23d02a1d7cbdc4cd7466513823c4c2" title="TickCallBack" alt="" coords="367,1043,465,1069"/>
</map>
