SRD Standelone programmation box: Globals

| SRD Standelone programmation box 2.0 (16/11/15 10:00:00) Documentation of the SRD standelone programmation box

- Main Page
- Data Structures
- Files

- File List
- Globals

- All
- Functions
- Variables
- Enumerations
- Enumerator
- Macros

- b
- c
- d
- f
- i
- l
- m
- p
- r
- u
- w

All Data Structures Files Functions Variables Enumerations Enumerator Macros Pages

### - b -

- BUTTON_PRESSED : button.h
- BUTTON_READ : button.h
- BUTTON_RELEASED : button.h
- BUTTON_WRITE : button.h
- BUTTONMANAGER_READY_FOR_LPM : ButtonManager.h
- BUTTONMANAGER_STATE_DISPLAY_LOG_ERROR : ButtonManager.h
- BUTTONMANAGER_STATE_DISPLAY_RFID_ERROR : ButtonManager.h
- BUTTONMANAGER_STATE_DISPLAY_RFID_READ : ButtonManager.h
- BUTTONMANAGER_STATE_DISPLAY_RFID_WRITE : ButtonManager.h
- BUTTONMANAGER_STATE_DISPLAY_RFID_WRITE_ERROR : ButtonManager.h
- BUTTONMANAGER_STATE_DISPLAY_WAIT_TIME : ButtonManager.h
- BUTTONMANAGER_STATE_FINISH : ButtonManager.h
- BUTTONMANAGER_STATE_STANDBY : ButtonManager.h
- BUTTONMANAGER_STATE_START : ButtonManager.h
- BUTTONMANAGER_STATE_WAIT_RELEASE : ButtonManager.h
- BUTTONMANAGER_STATE_WAIT_RFID : ButtonManager.h
- BUTTONMANAGER_WORKING : ButtonManager.h

### - c -

- CR95_EXT_CONNECTED : CR95UartMapper.h
- CR95_EXT_UNCONNECTED : CR95UartMapper.h
- CR95_SELECT_EXTERNAL : CR95UartMapper.h
- CR95_SELECT_INTERNAL : CR95UartMapper.h
- CR95HF_BridgeState_Finish : CR95HF.h
- CR95HF_BridgeState_Send : CR95HF.h
- CR95HF_BridgeState_Start : CR95HF.h
- CR95HF_BridgeState_WaitAnswer : CR95HF.h
- CR95HF_COMMAND_BRIDGE : CR95HF.h
- CR95HF_COMMAND_ECHO : CR95HF.h
- CR95HF_COMMAND_FIELD15693 : CR95HF.h
- CR95HF_COMMAND_FIELDOFF : CR95HF.h
- CR95HF_COMMAND_HIBERNATE : CR95HF.h
- CR95HF_COMMAND_NONE : CR95HF.h
- CR95HF_COMMAND_READ : CR95HF.h
- CR95HF_COMMAND_WRITE : CR95HF.h
- CR95HF_EchoState_Finish : CR95HF.h
- CR95HF_EchoState_Send : CR95HF.h
- CR95HF_EchoState_Start : CR95HF.h
- CR95HF_EchoState_WaitAnswer : CR95HF.h
- CR95HF_Field15693State_Finish : CR95HF.h
- CR95HF_Field15693State_Send : CR95HF.h
- CR95HF_Field15693State_Start : CR95HF.h
- CR95HF_Field15693State_WaitAnswer : CR95HF.h
- CR95HF_FieldOffState_Finish : CR95HF.h
- CR95HF_FieldOffState_Send : CR95HF.h
- CR95HF_FieldOffState_Start : CR95HF.h
- CR95HF_FieldOffState_WaitAnswer : CR95HF.h
- CR95HF_HibernateState_Finish : CR95HF.h
- CR95HF_HibernateState_Send : CR95HF.h
- CR95HF_HibernateState_Start : CR95HF.h
- CR95HF_HibernateState_WaitAnswer : CR95HF.h
- CR95HF_IS_BUSY : CR95HF.h
- CR95HF_IS_READY : CR95HF.h
- CR95HF_ReadState_Finish : CR95HF.h
- CR95HF_ReadState_Send : CR95HF.h
- CR95HF_ReadState_Start : CR95HF.h
- CR95HF_ReadState_WaitAnswer : CR95HF.h
- CR95HF_RETURN_BUSY : CR95HF.h
- CR95HF_RETURN_ECHO_ERROR : CR95HF.h
- CR95HF_RETURN_FIELD15693_ERROR : CR95HF.h
- CR95HF_RETURN_FIELDOFF_ERROR : CR95HF.h
- CR95HF_RETURN_HIBERNATE_ERROR : CR95HF.h
- CR95HF_RETURN_OK : CR95HF.h
- CR95HF_RETURN_READ_ERROR : CR95HF.h
- CR95HF_RETURN_STATEMACHINE_ERROR : CR95HF.h
- CR95HF_RETURN_WORKING : CR95HF.h
- CR95HF_RETURN_WRITE_ERROR : CR95HF.h
- CR95HF_WriteState_Finish : CR95HF.h
- CR95HF_WriteState_Send : CR95HF.h
- CR95HF_WriteState_Start : CR95HF.h
- CR95HF_WriteState_WaitAnswer : CR95HF.h

### - d -

- DISPLAY_16SEG_1_ID : display.h
- DISPLAY_7SEG_1_ID : display.h
- DISPLAY_7SEG_2_ID : display.h
- DISPLAY_7SEG_3_ID : display.h
- DISPLAY_CMD_OFF : display.h
- DISPLAY_CMD_ON : display.h
- DISPLAY_POWER_OFF : display.h
- DISPLAY_POWER_ON : display.h

### - f -

- FM25V20_ALLOW_WRITE : FM25V20.h
- FM25V20_FORBIDDEN_WRITE : FM25V20.h
- FM25V20_HOLD_OFF : FM25V20.h
- FM25V20_HOLD_ON : FM25V20.h
- FM25V20_LowPowerMode : FM25V20.h
- FM25V20_WorkingMode : FM25V20.h
- FM25V20_WP_OFF : FM25V20.h
- FM25V20_WP_ON : FM25V20.h

### - i -

- I2C_ACK : i2c_common.h
- I2C_DATADIR_RECEIVE : i2c_common.h
- I2C_DATADIR_TRANSMIT : i2c_common.h
- I2C_NACK : i2c_common.h

### - l -

- LED_GREEN : led.h
- LED_OFF : led.h
- LED_ON : led.h
- LED_RED : led.h
- LTC_CHARGER_isCharging : LTC4160.h
- LTC_CHARGER_isNotCharging : LTC4160.h
- LTC_FAULT_FaultPending : LTC4160.h
- LTC_FAULT_ok : LTC4160.h
- LTC_VBUS_VBusError : LTC4160.h
- LTC_VBUS_VBusGood : LTC4160.h
- LtcEncharger_OFF : LTC4160.h
- LtcEncharger_ON : LTC4160.h
- LTCUSBCurrent10xMode : LTC4160.h
- LTCUSBCurrent1xMode : LTC4160.h
- LTCUSBCurrent5xMode : LTC4160.h
- LTCUSBCurrentLPMode : LTC4160.h

### - m -

- MEMORYMANAGER_READ_OPERATION : MemoryManager.h
- MEMORYMANAGER_WRITE_OPERATION : MemoryManager.h

### - p -

- PIT_MODULE0 : pit.h
- PIT_MODULE1 : pit.h

### - r -

- RFID_HIBERNATE : RFIDManager.h
- RFID_POWERED : RFIDManager.h
- RFID_READY_FOR_LPM : RFIDManager.h
- RFID_RESULT_BRIDGE_ERROR : RFIDManager.h
- RFID_RESULT_EXTLPM_ERROR : RFIDManager.h
- RFID_RESULT_INTLPM_ERROR : RFIDManager.h
- RFID_RESULT_OK : RFIDManager.h
- RFID_RESULT_READ_ERROR : RFIDManager.h
- RFID_RESULT_WRITE_ERROR : RFIDManager.h
- RFID_STATE_BRIDGE : RFIDManager.h
- RFID_State_Bridge_Antenna : RFIDManager.h
- RFID_State_Bridge_Echo : RFIDManager.h
- RFID_State_Bridge_FieldOn : RFIDManager.h
- RFID_State_Bridge_Finish : RFIDManager.h
- RFID_State_Bridge_SendError : RFIDManager.h
- RFID_State_Bridge_SendResult : RFIDManager.h
- RFID_State_Bridge_Start : RFIDManager.h
- RFID_State_Bridge_Transfert : RFIDManager.h
- RFID_State_Bridge_WaitAntenna : RFIDManager.h
- RFID_State_Bridge_WaitEcho : RFIDManager.h
- RFID_State_Bridge_WaitFieldOn : RFIDManager.h
- RFID_State_Bridge_WaitTransfert : RFIDManager.h
- RFID_State_ExtLpm_Echo : RFIDManager.h
- RFID_State_ExtLpm_FieldOff : RFIDManager.h
- RFID_State_ExtLpm_Finish : RFIDManager.h
- RFID_State_ExtLpm_Hibernate : RFIDManager.h
- RFID_State_ExtLpm_Start : RFIDManager.h
- RFID_State_ExtLpm_WaitEcho : RFIDManager.h
- RFID_State_ExtLpm_WaitFieldOff : RFIDManager.h
- RFID_State_ExtLpm_WaitHibernate : RFIDManager.h
- RFID_State_IntLpm_Echo : RFIDManager.h
- RFID_State_IntLpm_FieldOff : RFIDManager.h
- RFID_State_IntLpm_Finish : RFIDManager.h
- RFID_State_IntLpm_Hibernate : RFIDManager.h
- RFID_State_IntLpm_Start : RFIDManager.h
- RFID_State_IntLpm_WaitEcho : RFIDManager.h
- RFID_State_IntLpm_WaitFieldOff : RFIDManager.h
- RFID_State_IntLpm_WaitHibernate : RFIDManager.h
- RFID_STATE_LOW_POWER_EXT : RFIDManager.h
- RFID_STATE_LOW_POWER_INT : RFIDManager.h
- RFID_STATE_READ : RFIDManager.h
- RFID_State_Read_Antenna : RFIDManager.h
- RFID_State_Read_Echo : RFIDManager.h
- RFID_State_Read_FieldOn : RFIDManager.h
- RFID_State_Read_Finish : RFIDManager.h
- RFID_State_Read_Read : RFIDManager.h
- RFID_State_Read_Start : RFIDManager.h
- RFID_State_Read_WaitAntenna : RFIDManager.h
- RFID_State_Read_WaitEcho : RFIDManager.h
- RFID_State_Read_WaitFieldOn : RFIDManager.h
- RFID_State_Read_WaitRead : RFIDManager.h
- RFID_STATE_STANDBY : RFIDManager.h
- RFID_STATE_WRITE : RFIDManager.h
- RFID_State_Write_Antenna : RFIDManager.h
- RFID_State_Write_Echo : RFIDManager.h
- RFID_State_Write_FieldOn : RFIDManager.h
- RFID_State_Write_Finish : RFIDManager.h
- RFID_State_Write_IsWritable : RFIDManager.h
- RFID_State_Write_Lock : RFIDManager.h
- RFID_State_Write_Read : RFIDManager.h
- RFID_State_Write_ReadSerial : RFIDManager.h
- RFID_State_Write_Start : RFIDManager.h
- RFID_State_Write_Unlock : RFIDManager.h
- RFID_State_Write_WaitAntenna : RFIDManager.h
- RFID_State_Write_WaitEcho : RFIDManager.h
- RFID_State_Write_WaitFieldOn : RFIDManager.h
- RFID_State_Write_WaitLock : RFIDManager.h
- RFID_State_Write_WaitRead : RFIDManager.h
- RFID_State_Write_WaitReadSerial : RFIDManager.h
- RFID_State_Write_WaitUnlock : RFIDManager.h
- RFID_State_Write_WaitWrite : RFIDManager.h
- RFID_State_Write_WaitWriteChecksum : RFIDManager.h
- RFID_State_Write_Write : RFIDManager.h
- RFID_State_Write_WriteChecksum : RFIDManager.h
- RFID_WORKING : RFIDManager.h

### - u -

- UsbCmdProtocole : UsbManager.h
- UsbCmdRemote : UsbManager.h
- UsbCmdRFIDEcho : UsbManager.h
- UsbCmdRw : UsbManager.h

### - w -

- WATCHDOG_PERIOD_LONG : watchdog.h
- WATCHDOG_PERIOD_MIDDLE : watchdog.h
- WATCHDOG_PERIOD_SHORT : watchdog.h
- WATCHDOG_SOURCE_CLOCK_BUS_CLOCK : watchdog.h
- WATCHDOG_SOURCE_CLOCK_LPO : watchdog.h