SRD Standelone programmation box: Data Structures

| SRD Standelone programmation box 2.0 (16/11/15 10:00:00) Documentation of the SRD standelone programmation box

- Main Page
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

All Data Structures Files Functions Variables Enumerations Enumerator Macros Pages
Data Structures
Here are the data structures with brief descriptions:

C t16SegDisplay | Structure used to control all segments in a 16 segments display
C t7SegDisplay | Structure used to control all segments in a 7 segments display
C tBQBatteryStatus | Struct used to store informations about the cell monitoring
C tButtonManagerCtrl | Button power manager mode
C tCR95HFCtrl | Define the structure used to control the CR95HF module
C tDeviceClock | Define clock source
C tFM25V20StatusReg | Structure used to read and get the status register of the device
C tMemoryManagerCtrl | Define a structure used to control the memory operation
C tMemoryManagerDiving | Define a structure used to save the diving parameters
C tMemoryManagerLog | Define a structure used to store a log in memory
C tMemoryManagerSerial | Define a structure used to save the serial parameters
C tMemTestErrorRecorder |
C tPowerManagerCtrl | Define a structure used by the power manager to control power modes
C tRFIDCtrl | Define a structure to control the RFID operation
C tSRDEeprom | Structure used to represent and store SRD RFID memory
C tTickCtrl | Structure used to control ticks
C tUartCtrl | Define the Uart control structure
C tUartFifo | Define the FIFO structure used by the uart controller
C tUartFlags | Define the Uart structure flags
C tUsbCtrl | Define a structure used by the USB Manager to control operation