<map id="ButtonManagerDisplayRfidError" name="ButtonManagerDisplayRfidError">
<area shape="rect" id="node2" href="$display_8c.html#a0529c896e4069df4bb7c4e767f36be28" title="Function used set the data displayed. " alt="" coords="230,132,399,159"/>
<area shape="rect" id="node8" href="$display_8c.html#a20d8e5860540ecfe3c0bb5a237bc17f8" title="Function used to enable/disable the display power. " alt="" coords="254,220,375,247"/>
<area shape="rect" id="node3" href="$display_8c.html#ace411722dfe7b549d16c09991a5ff24f" title="Function used to root 7 segments command on the rigth PIN. " alt="" coords="469,5,603,32"/>
<area shape="rect" id="node4" href="$decoder7_seg_8c.html#a8e8cab35cf7c9517f7094f42637a086e" title="Function used to decode a char and display it on a 7 segments digit. " alt="" coords="459,56,613,83"/>
<area shape="rect" id="node5" href="$display_8c.html#a771439bf50110fb999649ac3262bc4ef" title="Function used to root 16 segments command on the rigth PIN. " alt="" coords="465,107,607,133"/>
<area shape="rect" id="node6" href="$decoder16_seg_8c.html#a2d2fc41a03a66256e4681e8d695f01b0" title="Function used to decode a char and display it on a 16 segments digit. " alt="" coords="456,157,616,184"/>
<area shape="rect" id="node7" href="$spi0_8c.html#a6d528a26e3df5e8bdb80622df3946998" title="Function used to send data over the SPI module 0. " alt="" coords="497,232,575,259"/>
<area shape="rect" id="node9" href="$_d_s_p__mkl16z256vlh4_8c.html#ad30b60ccfc1302cb250629c495851333" title="Functions to MAP the defined IO of the SPI module x in the rigth pin. " alt="" coords="448,283,624,309"/>
</map>
