<map id="DisplaySetDataDisplayed" name="DisplaySetDataDisplayed">
<area shape="rect" id="node2" href="$decoder16_seg_8c.html#a2d2fc41a03a66256e4681e8d695f01b0" title="Function used to decode a char and display it on a 16 segments digit. " alt="" coords="224,5,384,32"/>
<area shape="rect" id="node3" href="$decoder7_seg_8c.html#a8e8cab35cf7c9517f7094f42637a086e" title="Function used to decode a char and display it on a 7 segments digit. " alt="" coords="227,56,381,83"/>
<area shape="rect" id="node4" href="$display_8c.html#a771439bf50110fb999649ac3262bc4ef" title="Function used to root 16 segments command on the rigth PIN. " alt="" coords="233,107,375,133"/>
<area shape="rect" id="node5" href="$display_8c.html#ace411722dfe7b549d16c09991a5ff24f" title="Function used to root 7 segments command on the rigth PIN. " alt="" coords="237,157,371,184"/>
<area shape="rect" id="node6" href="$spi0_8c.html#a6d528a26e3df5e8bdb80622df3946998" title="Function used to send data over the SPI module 0. " alt="" coords="265,232,343,259"/>
</map>
