<map id="PowerManagerInit" name="PowerManagerInit">
<area shape="rect" id="node2" href="$_b_q27510_d_r_z_r_g2_8c.html#a2cb45043dac162bf292c5613f6f9fe68" title="Function used to initialize the BQ device and it&#39;s DSP peripheral. " alt="" coords="234,31,385,57"/>
<area shape="rect" id="node6" href="$_l_t_c4160_8c.html#a6314c6a65847fe9ede22c7c54dee4029" title="Initialize the LTC4160 device. " alt="" coords="264,81,355,108"/>
<area shape="rect" id="node7" href="$_l_t_c4160_8c.html#a1859ad97d50351b41fa4ddad7ad928c8" title="Define the current limit drawn by the charger. " alt="" coords="247,132,371,159"/>
<area shape="rect" id="node8" href="$_power_manager_8c.html#ad82283ab9a30920f56833e7d42dd66c8" title="PowerManagerClearWakeUpInterruptFlag" alt="" coords="179,183,439,209"/>
<area shape="rect" id="node3" href="$i2c0_8c.html#afb1f62a78531bcfd5f2081d1b64e43ad" title="Initialized the I2C0 module with the defined parameters. " alt="" coords="489,31,554,57"/>
<area shape="rect" id="node4" href="$_d_s_p__mkl16z256vlh4_8c.html#a5e21c411f7c8bdda9dc52bb6114ab9f4" title="Functions to enable/disable the main clock of the specified I2C. " alt="" coords="636,5,745,32"/>
<area shape="rect" id="node5" href="$_d_s_p__mkl16z256vlh4_8c.html#a5f699c7ddbcad4b8d84fa41305dfec3f" title="Functions to MAP the defined IO of the I2C module x in the rigth pin. " alt="" coords="603,56,778,83"/>
</map>
