<map id="task1s" name="task1s">
<area shape="rect" id="node2" href="$_power_manager_8c.html#a611c841c363bb8044e88747cc39e7c30" title="power manager. " alt="" coords="115,940,223,967"/>
<area shape="rect" id="node3" href="$_b_q27510_d_r_z_r_g2_8c.html#ab6764798c058c46b3cdcf21c97027ffb" title="Function used to get all information about the cell monitoring. " alt="" coords="317,459,424,486"/>
<area shape="rect" id="node24" href="$_power_manager_8c.html#aa781287c32b2238935eb53a6ce806419" title="PowerManagerDisplayLoading" alt="" coords="273,966,469,992"/>
<area shape="rect" id="node34" href="$_power_manager_8c.html#a20ccb5a44ea9c3ecb98d6ec3ed84c62a" title="PowerManagerDisplayLoading\lError" alt="" coords="273,1017,469,1058"/>
<area shape="rect" id="node35" href="$_power_manager_8c.html#a851ecff0a5e93c3b261accadbf32621b" title="PowerManagerDisplayLoaded" alt="" coords="274,915,467,942"/>
<area shape="rect" id="node4" href="$_b_q27510_d_r_z_r_g2_8c.html#ab9dcad56c77f04971532555567a0d84b" title="Function used to know if a battery is connected or not. " alt="" coords="789,180,949,207"/>
<area shape="rect" id="node6" href="$_b_q27510_d_r_z_r_g2_8c.html#ac5d4fef49e298779b1753f40cf601cd3" title="BQ_getAvailableEnergy" alt="" coords="546,256,705,283"/>
<area shape="rect" id="node8" href="$_b_q27510_d_r_z_r_g2_8c.html#a9854bebed505691984f1cfa674cb3cb1" title="BQ_getAverageCurrent" alt="" coords="548,307,703,334"/>
<area shape="rect" id="node9" href="$_b_q27510_d_r_z_r_g2_8c.html#a28acfc3f3d1ff8e9d9d91edadc29ecd5" title="BQ_getAveragePower" alt="" coords="551,358,699,384"/>
<area shape="rect" id="node10" href="$_b_q27510_d_r_z_r_g2_8c.html#af8268e396eeb7abdfb21a7fbf03f1396" title="Function used to get some information about the cell monitoring. " alt="" coords="545,408,705,435"/>
<area shape="rect" id="node11" href="$_b_q27510_d_r_z_r_g2_8c.html#af6d8cc1ca065bcb90798788851de572c" title="BQ_getCellVoltage" alt="" coords="559,459,691,486"/>
<area shape="rect" id="node12" href="$_b_q27510_d_r_z_r_g2_8c.html#a02b013ae0aec405f9c7ceb909199f5f0" title="BQ_getCycleCount" alt="" coords="559,510,692,536"/>
<area shape="rect" id="node13" href="$_b_q27510_d_r_z_r_g2_8c.html#aaead900b00cb48e635c7db154f99c3e5" title="BQ_getFullAvailableCapacity" alt="" coords="531,560,720,587"/>
<area shape="rect" id="node14" href="$_b_q27510_d_r_z_r_g2_8c.html#a148f18dc993b083cacc31ff1f4dc71ed" title="BQ_getFullChargeCapacity" alt="" coords="536,611,715,638"/>
<area shape="rect" id="node15" href="$_b_q27510_d_r_z_r_g2_8c.html#a42dac1127d0914053de05fd9af45b77a" title="BQ_getMaxLoadCurrent" alt="" coords="545,662,706,688"/>
<area shape="rect" id="node16" href="$_b_q27510_d_r_z_r_g2_8c.html#aa723c8cc7b39b74ae4c344cb39350aed" title="BQ_getMaxLoadTimeToEmpty" alt="" coords="526,712,725,739"/>
<area shape="rect" id="node17" href="$_b_q27510_d_r_z_r_g2_8c.html#a14b533c028c320fc9b2a5b9043d0e259" title="BQ_getNominalAvailableCapacity" alt="" coords="518,763,733,790"/>
<area shape="rect" id="node18" href="$_b_q27510_d_r_z_r_g2_8c.html#a6602062ce84e9142bfab316784516eb8" title="BQ_getRemainingCapacity" alt="" coords="536,814,715,840"/>
<area shape="rect" id="node19" href="$_b_q27510_d_r_z_r_g2_8c.html#a3a21f0765f44c716b638d8b8773946d2" title="BQ_getStandbyTimeToEmpty" alt="" coords="528,864,723,891"/>
<area shape="rect" id="node20" href="$_b_q27510_d_r_z_r_g2_8c.html#a84d862a65a34dff063b11338b89a5931" title="BQ_getStateOfCharge" alt="" coords="550,54,701,80"/>
<area shape="rect" id="node21" href="$_b_q27510_d_r_z_r_g2_8c.html#ab0c39d16ad675e6a83e2659c9a51551b" title="BQ_getTimeToEmpty" alt="" coords="552,104,699,131"/>
<area shape="rect" id="node22" href="$_b_q27510_d_r_z_r_g2_8c.html#aade4e442c60a3cf1aa9223a7696483dc" title="BQ_getTimeToFull" alt="" coords="561,155,690,182"/>
<area shape="rect" id="node23" href="$_b_q27510_d_r_z_r_g2_8c.html#a8a62d091a91f6665acc0bd38ee9af9da" title="BQ_getTTEAtConstantPower" alt="" coords="530,206,721,232"/>
<area shape="rect" id="node5" href="$i2c0_8c.html#ada7d730a8793a6ddd23180047b309447" title="Send a packet on the I2C interface. " alt="" coords="1006,307,1085,334"/>
<area shape="rect" id="node7" href="$i2c0_8c.html#a1f3862c3506c31b0a50c7914f17314ab" title="Read a packet on the I2C interface. " alt="" coords="830,434,909,460"/>
<area shape="rect" id="node25" href="$display_8c.html#ad8f9098d6f81dbce9ff70ef99662f212" title="Function used get the data displayed. " alt="" coords="540,915,711,942"/>
<area shape="rect" id="node26" href="$display_8c.html#a20d8e5860540ecfe3c0bb5a237bc17f8" title="Function used to enable/disable the display power. " alt="" coords="565,1024,686,1051"/>
<area shape="rect" id="node28" href="$display_8c.html#a0529c896e4069df4bb7c4e767f36be28" title="Function used set the data displayed. " alt="" coords="541,966,710,992"/>
<area shape="rect" id="node27" href="$_d_s_p__mkl16z256vlh4_8c.html#ad30b60ccfc1302cb250629c495851333" title="Functions to MAP the defined IO of the SPI module x in the rigth pin. " alt="" coords="781,1104,957,1131"/>
<area shape="rect" id="node29" href="$decoder16_seg_8c.html#a2d2fc41a03a66256e4681e8d695f01b0" title="Function used to decode a char and display it on a 16 segments digit. " alt="" coords="789,1054,949,1080"/>
<area shape="rect" id="node30" href="$decoder7_seg_8c.html#a8e8cab35cf7c9517f7094f42637a086e" title="Function used to decode a char and display it on a 7 segments digit. " alt="" coords="793,827,946,854"/>
<area shape="rect" id="node31" href="$display_8c.html#a771439bf50110fb999649ac3262bc4ef" title="Function used to root 16 segments command on the rigth PIN. " alt="" coords="798,878,941,904"/>
<area shape="rect" id="node32" href="$display_8c.html#ace411722dfe7b549d16c09991a5ff24f" title="Function used to root 7 segments command on the rigth PIN. " alt="" coords="802,928,937,955"/>
<area shape="rect" id="node33" href="$spi0_8c.html#a6d528a26e3df5e8bdb80622df3946998" title="Function used to send data over the SPI module 0. " alt="" coords="830,1003,909,1030"/>
</map>
