<map id="BQ_getFullInfo" name="BQ_getFullInfo">
<area shape="rect" id="node2" href="$_b_q27510_d_r_z_r_g2_8c.html#ab9dcad56c77f04971532555567a0d84b" title="Function used to know if a battery is connected or not. " alt="" coords="424,182,584,209"/>
<area shape="rect" id="node4" href="$_b_q27510_d_r_z_r_g2_8c.html#ac5d4fef49e298779b1753f40cf601cd3" title="BQ_getAvailableEnergy" alt="" coords="189,55,347,82"/>
<area shape="rect" id="node6" href="$_b_q27510_d_r_z_r_g2_8c.html#a9854bebed505691984f1cfa674cb3cb1" title="BQ_getAverageCurrent" alt="" coords="191,106,345,133"/>
<area shape="rect" id="node7" href="$_b_q27510_d_r_z_r_g2_8c.html#a28acfc3f3d1ff8e9d9d91edadc29ecd5" title="BQ_getAveragePower" alt="" coords="194,157,342,183"/>
<area shape="rect" id="node8" href="$_b_q27510_d_r_z_r_g2_8c.html#af8268e396eeb7abdfb21a7fbf03f1396" title="Function used to get some information about the cell monitoring. " alt="" coords="188,207,348,234"/>
<area shape="rect" id="node9" href="$_b_q27510_d_r_z_r_g2_8c.html#af6d8cc1ca065bcb90798788851de572c" title="BQ_getCellVoltage" alt="" coords="202,258,334,285"/>
<area shape="rect" id="node10" href="$_b_q27510_d_r_z_r_g2_8c.html#a02b013ae0aec405f9c7ceb909199f5f0" title="BQ_getCycleCount" alt="" coords="201,309,335,335"/>
<area shape="rect" id="node11" href="$_b_q27510_d_r_z_r_g2_8c.html#aaead900b00cb48e635c7db154f99c3e5" title="BQ_getFullAvailableCapacity" alt="" coords="173,359,363,386"/>
<area shape="rect" id="node12" href="$_b_q27510_d_r_z_r_g2_8c.html#a148f18dc993b083cacc31ff1f4dc71ed" title="BQ_getFullChargeCapacity" alt="" coords="179,410,357,437"/>
<area shape="rect" id="node13" href="$_b_q27510_d_r_z_r_g2_8c.html#a42dac1127d0914053de05fd9af45b77a" title="BQ_getMaxLoadCurrent" alt="" coords="187,461,349,487"/>
<area shape="rect" id="node14" href="$_b_q27510_d_r_z_r_g2_8c.html#aa723c8cc7b39b74ae4c344cb39350aed" title="BQ_getMaxLoadTimeToEmpty" alt="" coords="169,511,367,538"/>
<area shape="rect" id="node15" href="$_b_q27510_d_r_z_r_g2_8c.html#a14b533c028c320fc9b2a5b9043d0e259" title="BQ_getNominalAvailableCapacity" alt="" coords="161,562,375,589"/>
<area shape="rect" id="node16" href="$_b_q27510_d_r_z_r_g2_8c.html#a6602062ce84e9142bfab316784516eb8" title="BQ_getRemainingCapacity" alt="" coords="179,613,357,639"/>
<area shape="rect" id="node17" href="$_b_q27510_d_r_z_r_g2_8c.html#a3a21f0765f44c716b638d8b8773946d2" title="BQ_getStandbyTimeToEmpty" alt="" coords="171,663,365,690"/>
<area shape="rect" id="node18" href="$_b_q27510_d_r_z_r_g2_8c.html#a84d862a65a34dff063b11338b89a5931" title="BQ_getStateOfCharge" alt="" coords="193,714,343,741"/>
<area shape="rect" id="node19" href="$_b_q27510_d_r_z_r_g2_8c.html#ab0c39d16ad675e6a83e2659c9a51551b" title="BQ_getTimeToEmpty" alt="" coords="195,765,341,791"/>
<area shape="rect" id="node20" href="$_b_q27510_d_r_z_r_g2_8c.html#aade4e442c60a3cf1aa9223a7696483dc" title="BQ_getTimeToFull" alt="" coords="203,815,333,842"/>
<area shape="rect" id="node21" href="$_b_q27510_d_r_z_r_g2_8c.html#a8a62d091a91f6665acc0bd38ee9af9da" title="BQ_getTTEAtConstantPower" alt="" coords="173,866,363,893"/>
<area shape="rect" id="node3" href="$i2c0_8c.html#ada7d730a8793a6ddd23180047b309447" title="Send a packet on the I2C interface. " alt="" coords="633,309,711,335"/>
<area shape="rect" id="node5" href="$i2c0_8c.html#a1f3862c3506c31b0a50c7914f17314ab" title="Read a packet on the I2C interface. " alt="" coords="465,435,543,462"/>
</map>
