<map id="taskBackground" name="taskBackground">
<area shape="rect" id="node2" href="$_button_manager_8c.html#a6131a6127b6045f5c352ca091ebdb36a" title="Button manager function. " alt="" coords="326,283,437,309"/>
<area shape="rect" id="node28" href="$_power_manager_8c.html#aef7050cf231cfdbbdb4134de79e10add" title="Low Power mode controller. " alt="" coords="491,728,682,755"/>
<area shape="rect" id="node40" href="$_r_f_i_d_manager_8c.html#a6615b2f62061cbe70614f874e2edd1c5" title="RFID manager. " alt="" coords="171,1133,272,1160"/>
<area shape="rect" id="node49" href="$_usb_manager_8c.html#a1e480179c92fe988f89777f353e9ef9a" title="USB manager. " alt="" coords="334,905,429,932"/>
<area shape="rect" id="node3" href="$_button_manager_8c.html#afdd019b240e44a51aba9069b09cd3ee8" title="ButtonManagerDealer" alt="" coords="513,539,660,565"/>
<area shape="rect" id="node5" href="$display_8c.html#a0529c896e4069df4bb7c4e767f36be28" title="Function used set the data displayed. " alt="" coords="1022,295,1191,321"/>
<area shape="rect" id="node11" href="$display_8c.html#a20d8e5860540ecfe3c0bb5a237bc17f8" title="Function used to enable/disable the display power. " alt="" coords="1046,357,1167,384"/>
<area shape="rect" id="node21" href="$tick_8c.html#aa43bd4bc67b26f7e7ab31be06b088a14" title="Get the milliseconds counter. " alt="" coords="1041,1108,1172,1135"/>
<area shape="rect" id="node22" href="$tick_8c.html#a0145cffb9b0238336157774cbdb484a9" title="Get the milliseconds counter. " alt="" coords="759,1108,929,1135"/>
<area shape="rect" id="node23" href="$_button_manager_8c.html#a72f46a32970390d2c24e0e177d3d7985" title="ButtonManagerDisplayDate\lError" alt="" coords="754,158,934,199"/>
<area shape="rect" id="node24" href="$_button_manager_8c.html#a46d3f9715cc22d9bb745d0971b137094" title="ButtonManagerDisplayNone" alt="" coords="753,224,935,251"/>
<area shape="rect" id="node25" href="$_button_manager_8c.html#ac9681c8a673eea2c004dcd6838accb03" title="ButtonManagerDisplayProgrammed\lError" alt="" coords="731,275,957,317"/>
<area shape="rect" id="node26" href="$display_8c.html#ad8f9098d6f81dbce9ff70ef99662f212" title="Function used get the data displayed. " alt="" coords="501,5,672,32"/>
<area shape="rect" id="node27" href="$rtc_8c.html#acc23a8b28879660bbc371e432dd1c140" title="Indicate if the RTC have been initialized or not. " alt="" coords="495,56,678,83"/>
<area shape="rect" id="node4" href="$_button_manager_8c.html#a9e4446b1a305b75138f80df13ca38f26" title="ButtonManagerDisplayLogError" alt="" coords="743,341,945,368"/>
<area shape="rect" id="node13" href="$_button_manager_8c.html#a9afe02c03b610c40e5d86a88873f0b65" title="ButtonManagerDisplayRead" alt="" coords="753,392,935,419"/>
<area shape="rect" id="node14" href="$_button_manager_8c.html#ab2d0aabb7a374961991dd4a80c0c9654" title="ButtonManagerDisplayRfid\lError" alt="" coords="757,443,931,485"/>
<area shape="rect" id="node15" href="$_button_manager_8c.html#ae2f1b19b0a4b64760e2fe56761fadb76" title="ButtonManagerDisplayWrite" alt="" coords="752,509,936,536"/>
<area shape="rect" id="node16" href="$_button_manager_8c.html#a7467a0fb45a4b96ba5e07000b94aaeea" title="ButtonManagerDisplayWrite\lError" alt="" coords="752,561,936,602"/>
<area shape="rect" id="node17" href="$_memory_manager_8c.html#aaf68fcb13458866a83fe16fa9c66aca9" title="function used read/write and check the log in the memory. " alt="" coords="759,779,929,805"/>
<area shape="rect" id="node20" href="$rtc_8c.html#a12763edd744e1e2eb152fc965e0705d6" title="return the current time in the RTC. " alt="" coords="799,880,889,907"/>
<area shape="rect" id="node6" href="$decoder16_seg_8c.html#a2d2fc41a03a66256e4681e8d695f01b0" title="Function used to decode a char and display it on a 16 segments digit. " alt="" coords="1307,256,1467,283"/>
<area shape="rect" id="node7" href="$decoder7_seg_8c.html#a8e8cab35cf7c9517f7094f42637a086e" title="Function used to decode a char and display it on a 7 segments digit. " alt="" coords="1310,307,1463,333"/>
<area shape="rect" id="node8" href="$display_8c.html#a771439bf50110fb999649ac3262bc4ef" title="Function used to root 16 segments command on the rigth PIN. " alt="" coords="1315,357,1458,384"/>
<area shape="rect" id="node9" href="$display_8c.html#ace411722dfe7b549d16c09991a5ff24f" title="Function used to root 7 segments command on the rigth PIN. " alt="" coords="1319,131,1454,157"/>
<area shape="rect" id="node10" href="$spi0_8c.html#a6d528a26e3df5e8bdb80622df3946998" title="Function used to send data over the SPI module 0. " alt="" coords="1347,205,1426,232"/>
<area shape="rect" id="node12" href="$_d_s_p__mkl16z256vlh4_8c.html#ad30b60ccfc1302cb250629c495851333" title="Functions to MAP the defined IO of the SPI module x in the rigth pin. " alt="" coords="1299,408,1475,435"/>
<area shape="rect" id="node18" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="1053,947,1160,973"/>
<area shape="rect" id="node19" href="$_f_m25_v20_8c.html#ab71cea0f2db62d709c9b1a6441a70581" title="Put the memory in a low power mode. " alt="" coords="1054,997,1159,1024"/>
<area shape="rect" id="node29" href="$_power_manager_8c.html#a7406ccf39ad8768c5043ac74da94a63b" title="Functions used to Enter and exit low power mode. " alt="" coords="761,728,927,755"/>
<area shape="rect" id="node36" href="$_power_manager_8c.html#a1c56b577113fb8580a4f6fb0abe50fea" title="PowerManagerExitLPM" alt="" coords="765,677,923,704"/>
<area shape="rect" id="node30" href="$_d_s_p__mkl16z256vlh4_8c.html#aa0ebd2465a6d7946e08a90b6dd0dfd90" title="Functions to enable/disable the main clock of the specified uart. " alt="" coords="1045,779,1169,805"/>
<area shape="rect" id="node31" href="$_d_s_p__mkl16z256vlh4_8c.html#ade83ccc4c990b0da74572b7fbc556015" title="UART1ClockGate" alt="" coords="1045,677,1169,704"/>
<area shape="rect" id="node32" href="$_d_s_p__mkl16z256vlh4_8c.html#aaf402774cc148a8964baef5dfa2c0f63" title="UART2ClockGate" alt="" coords="1045,728,1169,755"/>
<area shape="rect" id="node33" href="$_power_manager_8c.html#a841a006cab2c35f157e9cb986a5ed4cf" title="Functions used to control the wake up interrupt functions. " alt="" coords="1007,830,1206,871"/>
<area shape="rect" id="node35" href="$device_8c.html#afc4edee1a81067e2cd15de38145be61e" title="Function to switch the device in very low power mode. " alt="" coords="1061,896,1152,923"/>
<area shape="rect" id="node34" href="$_power_manager_8c.html#ad82283ab9a30920f56833e7d42dd66c8" title="PowerManagerClearWakeUpInterruptFlag" alt="" coords="1257,732,1517,759"/>
<area shape="rect" id="node37" href="$_power_manager_8c.html#abc288b84841dcde78bcdb6f57da9d8d1" title="PowerManagerDisableWakeUp\lInterrupt" alt="" coords="1006,459,1207,501"/>
<area shape="rect" id="node38" href="$device_8c.html#a631a644dd7e158b7fa45c4bfe43b29bc" title="Function to switch the processor on the highest clock speed allowed. " alt="" coords="1009,525,1204,552"/>
<area shape="rect" id="node39" href="$_power_manager_8c.html#a611c841c363bb8044e88747cc39e7c30" title="power manager. " alt="" coords="1053,576,1161,603"/>
<area shape="rect" id="node41" href="$_c_r95_uart_mapper_8c.html#a7ad185503043b02e75769ae9ebb3e6b9" title="Return the connection state of the CR95HF module. " alt="" coords="749,1336,939,1363"/>
<area shape="rect" id="node42" href="$_r_f_i_d_manager_8c.html#ac7dc07d3fd12132286ea2fa1a90057b5" title="RFIDDealer" alt="" coords="337,1260,425,1287"/>
<area shape="rect" id="node48" href="$_c_r95_h_f_8c.html#ac51f39d982f31bb7548abf2bd31065b5" title="Global manager of the CR95HF module. " alt="" coords="321,1083,442,1109"/>
<area shape="rect" id="node43" href="$_r_f_i_d_manager_8c.html#a6ab6b8dd0e473d8fdf4a01c3ffbd7852" title="RFIDBridgeStateMachine" alt="" coords="503,1387,671,1413"/>
<area shape="rect" id="node44" href="$_r_f_i_d_manager_8c.html#a776bd19e29a44fe5b562330efe4b1808" title="RFIDReadStateMachine" alt="" coords="506,1235,667,1261"/>
<area shape="rect" id="node45" href="$_r_f_i_d_manager_8c.html#aa800930fc21149f77f2b93ece7ede47b" title="RFIDWriteStateMachine" alt="" coords="505,1336,668,1363"/>
<area shape="rect" id="node46" href="$_r_f_i_d_manager_8c.html#a76aaad614e4215dd0b1f0a55c91448ff" title="RFIDIntLpmStateMachine" alt="" coords="501,1184,672,1211"/>
<area shape="rect" id="node47" href="$_r_f_i_d_manager_8c.html#aaadf0da29bf3176eb69c6e8ec6e08a6b" title="RFIDExtLpmStateMachine" alt="" coords="499,1285,675,1312"/>
<area shape="rect" id="node50" href="$_usb_manager_8c.html#ac8d1502564dd3480fc417f834a13cec2" title="Function use to deal received command. " alt="" coords="507,880,666,907"/>
</map>
