SRD Standelone programmation box: Data Fields

| SRD Standelone programmation box 2.0 (16/11/15 10:00:00) Documentation of the SRD standelone programmation box

- Main Page
- Data Structures
- Files

- Data Structures
- Data Structure Index
- Data Fields

- All
- Variables

- a
- b
- c
- d
- e
- f
- g
- h
- i
- k
- l
- m
- n
- o
- p
- r
- s
- t
- u
- v
- w

All Data Structures Files Functions Variables Enumerations Enumerator Macros Pages
Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - s -

- S : t16SegDisplay
- seg : t16SegDisplay , t7SegDisplay
- serial : tMemoryManagerCtrl , tMemoryManagerSerial
- serial0 : tSRDEeprom
- serial1 : tSRDEeprom
- serial2 : tSRDEeprom
- serial3 : tSRDEeprom
- serial4 : tSRDEeprom
- serial5 : tSRDEeprom
- serial6 : tSRDEeprom
- serial7 : tSRDEeprom
- serial8 : tSRDEeprom
- serial9 : tSRDEeprom
- sizeReceive : tCR95HFCtrl
- sizeReceived : tUsbCtrl
- srdData : tMemoryManagerLog
- SRDSerial1 : tSRDEeprom
- SRDSerial2 : tSRDEeprom
- SRDSerial3 : tSRDEeprom
- SRDSerial4 : tSRDEeprom
- SRDSerial5 : tSRDEeprom
- SRDSerial6 : tSRDEeprom
- SRDSerial7 : tSRDEeprom
- SRDSerial8 : tSRDEeprom
- standbyCurrent : tBQBatteryStatus
- standbyTimeToEmpty : tBQBatteryStatus
- state : tRFIDCtrl
- stateOfCharge : tBQBatteryStatus
- statusModule : tSRDEeprom
- stringReceived : tUartFlags
- subState : tRFIDCtrl
- supercap : tSRDEeprom
- systemClockFreq : tDeviceClock