<map id="main" name="main">
<area shape="rect" id="node2" href="$main_8c.html#a040d63354f4112c7ec2ca4d3a86a5b4a" title="Function used to initialize some critical peripheral. " alt="" coords="139,132,218,159"/>
<area shape="rect" id="node7" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="885,411,992,437"/>
<area shape="rect" id="node9" href="$main_8c.html#aadf3292d1b050137201649db87e63aa5" title="Function used to initialize all non critical peripheral. " alt="" coords="151,917,207,944"/>
<area shape="rect" id="node35" href="$main_8c.html#a02839675952784c88099f3519c8a5a1d" title="Function used to start scheduling operations. " alt="" coords="121,1069,236,1096"/>
<area shape="rect" id="node36" href="$main_8c.html#abc513c77d3ae6919b5983e6564643c11" title="Periodic tasks. " alt="" coords="135,1120,222,1147"/>
<area shape="rect" id="node37" href="$main_8c.html#aa472742a7516d3d5fcdc9c19a318dde9" title="Periodic tasks. " alt="" coords="139,1171,218,1197"/>
<area shape="rect" id="node38" href="$main_8c.html#a0f16db5a9799dbdc8a000444f323d9c1" title="Periodic tasks. " alt="" coords="141,1221,216,1248"/>
<area shape="rect" id="node39" href="$main_8c.html#a002a2c4d2546db675a7d4d74cdc7f277" title="Periodic tasks. " alt="" coords="148,968,209,995"/>
<area shape="rect" id="node45" href="$main_8c.html#a47b19cb17359b8a4930e1db6207395fb" title="Function used to deal background task. " alt="" coords="341,1491,457,1517"/>
<area shape="rect" id="node50" href="$main_8c.html#a8f2f419ec2126a9fb31399be60996cb0" title="Function used to deal task overrun. " alt="" coords="104,1272,253,1299"/>
<area shape="rect" id="node3" href="$device_8c.html#a631a644dd7e158b7fa45c4bfe43b29bc" title="Function to switch the processor on the highest clock speed allowed. " alt="" coords="301,157,496,184"/>
<area shape="rect" id="node4" href="$device_8c.html#a9237af6f7adfd2b81439ae8542694b8b" title="Function to initialize the device clock. " alt="" coords="360,5,437,32"/>
<area shape="rect" id="node6" href="$rtc_8c.html#aa884644b359833678d1f4bde7c214e32" title="Function used to initialized the RTC module. " alt="" coords="369,56,428,83"/>
<area shape="rect" id="node8" href="$watchdog_8c.html#a4f58d14b66f9b050c560664b217964d7" title="start watchdog (can be call only ones and can&#39;t call after WatchdogStop()). " alt="" coords="344,107,453,133"/>
<area shape="rect" id="node5" href="$device_8c.html#af0b6ea9b67bd97df7598273a732fedeb" title="Function to switch the processor clock on the FEI clock source. " alt="" coords="579,5,771,32"/>
<area shape="rect" id="node10" href="$_power_manager_8c.html#a6fc2f38d8cafdafb419605fddc230248" title="Variable used by the power manager. " alt="" coords="336,816,461,843"/>
<area shape="rect" id="node15" href="$led_8c.html#a1d5b4eaf7f01ae9557ba620158ebdfd9" title="Function used to initialize the leds. " alt="" coords="369,512,429,539"/>
<area shape="rect" id="node16" href="$_button_manager_8c.html#ae84a2c976c6278b78207e3ec6c6a2533" title="Function used to initialize the button manager. " alt="" coords="335,917,462,944"/>
<area shape="rect" id="node18" href="$_r_f_i_d_manager_8c.html#a67c55a98971bdbdc992fd3c60daebcc8" title="Function used to initialize the RFID manager. " alt="" coords="339,968,458,995"/>
<area shape="rect" id="node20" href="$tick_8c.html#a85de8acefef2c29ca44aa9728de87f92" title="Function used to initialize the Tick module . " alt="" coords="367,1019,430,1045"/>
<area shape="rect" id="node23" href="$display_8c.html#ae2c5b80a65268def4100ad7a1683b196" title="Function used to initialized the display. " alt="" coords="633,1120,716,1147"/>
<area shape="rect" id="node27" href="$display_8c.html#a20d8e5860540ecfe3c0bb5a237bc17f8" title="Function used to enable/disable the display power. " alt="" coords="878,1280,999,1307"/>
<area shape="rect" id="node28" href="$_memory_manager_8c.html#a75f5428e07dbdaee7b7d024a3447da8b" title="function use to initialize the memory manager. " alt="" coords="331,563,467,589"/>
<area shape="rect" id="node11" href="$_l_t_c4160_8c.html#a6314c6a65847fe9ede22c7c54dee4029" title="Initialize the LTC4160 device. " alt="" coords="629,867,720,893"/>
<area shape="rect" id="node12" href="$_b_q27510_d_r_z_r_g2_8c.html#a2cb45043dac162bf292c5613f6f9fe68" title="Function used to initialize the BQ device and it&#39;s DSP peripheral. " alt="" coords="599,715,750,741"/>
<area shape="rect" id="node13" href="$_l_t_c4160_8c.html#a1859ad97d50351b41fa4ddad7ad928c8" title="Define the current limit drawn by the charger. " alt="" coords="613,765,737,792"/>
<area shape="rect" id="node14" href="$_power_manager_8c.html#ad82283ab9a30920f56833e7d42dd66c8" title="PowerManagerClearWakeUpInterruptFlag" alt="" coords="545,816,805,843"/>
<area shape="rect" id="node17" href="$button_8c.html#a30a1cff81be3c91e307685387401e863" title="Function used to initialized the buttons. " alt="" coords="636,917,713,944"/>
<area shape="rect" id="node19" href="$_c_r95_h_f_8c.html#a5a280da3bb75613fbb5e62854ec65e3a" title="Function used to initialize the CR95HF global manager. " alt="" coords="631,968,719,995"/>
<area shape="rect" id="node21" href="$pit_8c.html#a77b58f0272b0bdf0cc4d7705b4627c77" title="Initialize a PIT module. " alt="" coords="647,1069,702,1096"/>
<area shape="rect" id="node22" href="$tick_8c.html#a0e23d02a1d7cbdc4cd7466513823c4c2" title="TickCallBack" alt="" coords="625,1019,724,1045"/>
<area shape="rect" id="node24" href="$display_8c.html#a0529c896e4069df4bb7c4e767f36be28" title="Function used set the data displayed. " alt="" coords="854,1221,1023,1248"/>
<area shape="rect" id="node25" href="$spi0_8c.html#aed55957fe67d7fa37fe71657a3a23885" title="Function used to initialize the SPI0 module. " alt="" coords="906,1145,971,1172"/>
<area shape="rect" id="node26" href="$_d_s_p__mkl16z256vlh4_8c.html#ad30b60ccfc1302cb250629c495851333" title="Functions to MAP the defined IO of the SPI module x in the rigth pin. " alt="" coords="1072,1213,1248,1240"/>
<area shape="rect" id="node29" href="$_f_m25_v20_8c.html#a2e18e393748dca1da43e4e069bc4972f" title="Function used to initialize the FM25V20 memory. " alt="" coords="627,563,722,589"/>
<area shape="rect" id="node30" href="$_memory_manager_8c.html#a4dd1d910cde969a31ad009fcca1bb4a4" title="function used read/write and check the diving parameters in the memory. " alt="" coords="583,664,766,691"/>
<area shape="rect" id="node31" href="$_memory_manager_8c.html#a23afd9881c251d81c7ff88b4fefbb8e4" title="MemoryManagerCheckDiving" alt="" coords="579,613,770,640"/>
<area shape="rect" id="node32" href="$_memory_manager_8c.html#a7161fed197cb374280e918eafb4d39a9" title="function used read/write and check the serial parameters in the memory. " alt="" coords="583,411,766,437"/>
<area shape="rect" id="node33" href="$_memory_manager_8c.html#a7b3973e4132860fb79b75c73bc111a6f" title="MemoryManagerCheckSerial" alt="" coords="580,360,769,387"/>
<area shape="rect" id="node34" href="$_memory_manager_8c.html#a95c0f9ae110105c19fb6eb0da09930e0" title="Return the number of log stored in memory. " alt="" coords="569,461,781,488"/>
<area shape="rect" id="node40" href="$_power_manager_8c.html#a611c841c363bb8044e88747cc39e7c30" title="power manager. " alt="" coords="345,1221,453,1248"/>
<area shape="rect" id="node41" href="$_b_q27510_d_r_z_r_g2_8c.html#ab6764798c058c46b3cdcf21c97027ffb" title="Function used to get all information about the cell monitoring. " alt="" coords="621,1339,728,1365"/>
<area shape="rect" id="node42" href="$_power_manager_8c.html#aa781287c32b2238935eb53a6ce806419" title="PowerManagerDisplayLoading" alt="" coords="577,1221,773,1248"/>
<area shape="rect" id="node43" href="$_power_manager_8c.html#a20ccb5a44ea9c3ecb98d6ec3ed84c62a" title="PowerManagerDisplayLoading\lError" alt="" coords="577,1273,773,1314"/>
<area shape="rect" id="node44" href="$_power_manager_8c.html#a851ecff0a5e93c3b261accadbf32621b" title="PowerManagerDisplayLoaded" alt="" coords="578,1171,771,1197"/>
<area shape="rect" id="node46" href="$_usb_manager_8c.html#a1e480179c92fe988f89777f353e9ef9a" title="USB manager. " alt="" coords="627,1491,722,1517"/>
<area shape="rect" id="node47" href="$_button_manager_8c.html#a6131a6127b6045f5c352ca091ebdb36a" title="Button manager function. " alt="" coords="619,1440,730,1467"/>
<area shape="rect" id="node48" href="$_r_f_i_d_manager_8c.html#a6615b2f62061cbe70614f874e2edd1c5" title="RFID manager. " alt="" coords="624,1541,725,1568"/>
<area shape="rect" id="node49" href="$_power_manager_8c.html#aef7050cf231cfdbbdb4134de79e10add" title="Low Power mode controller. " alt="" coords="579,1592,770,1619"/>
</map>
