<map id="Spi1Read" name="Spi1Read">
<area shape="rect" id="node2" href="$_f_m25_v20_8h.html#ace631f94926ad79e89fdfd13013659e6" title="Read data from the memory. " alt="" coords="279,233,414,260"/>
<area shape="rect" id="node20" href="$_f_m25_v20_8h.html#a81989bd9510f8ae046048c184c04feb2" title="Function used to read the device ID. " alt="" coords="269,321,425,348"/>
<area shape="rect" id="node21" href="$_f_m25_v20_8h.html#a35cd894c50c66a2bc5ebd81ab26bcfcf" title="Functions used to set and read the status register. " alt="" coords="262,372,431,399"/>
<area shape="rect" id="node22" href="$spi1_8h.html#a93ecc3b36648270cd041dad2bd467745" title="Function used to read data over the SPI module 1. " alt="" coords="134,289,213,316"/>
<area shape="rect" id="node3" href="$_f_m25_v20_mem_test_8h.html#a31b1c7bd95f8fc629c82fedbc7e86c19" title="FM25V20MemTest_Clear" alt="" coords="507,5,677,32"/>
<area shape="rect" id="node5" href="$_f_m25_v20_mem_test_8h.html#a5324c46da6daa18c72d434ddd2695b87" title="FM25V20MemTest_HighFreqDown" alt="" coords="481,56,703,83"/>
<area shape="rect" id="node6" href="$_f_m25_v20_mem_test_8h.html#a3dab3a8f4d5b585ffc341132a8905a4e" title="FM25V20MemTest_HighFreqUp" alt="" coords="489,107,695,133"/>
<area shape="rect" id="node7" href="$_f_m25_v20_mem_test_8h.html#aa801df1c3fb82c4b63ea3da6209ac73d" title="FM25V20MemTest_PulseN" alt="" coords="501,157,683,184"/>
<area shape="rect" id="node8" href="$_f_m25_v20_mem_test_8h.html#a5a0a75083ba30546c433ecb0b12edf3d" title="FM25V20MemTest_PulseP" alt="" coords="501,208,683,235"/>
<area shape="rect" id="node9" href="$_f_m25_v20_mem_test_8h.html#a4fa08b2f438caece8e0907091a74496f" title="FM25V20MemTest_Set" alt="" coords="513,259,671,285"/>
<area shape="rect" id="node10" href="$_memory_manager_8h.html#a95c0f9ae110105c19fb6eb0da09930e0" title="Return the number of log stored in memory. " alt="" coords="486,309,698,336"/>
<area shape="rect" id="node14" href="$_memory_manager_8h.html#a4dd1d910cde969a31ad009fcca1bb4a4" title="function used read/write and check the diving parameters in the memory. " alt="" coords="501,360,683,387"/>
<area shape="rect" id="node15" href="$_memory_manager_8h.html#a4621c0be0193d08ee84b8dc8bdaea778" title="function used read/write and check the log in the memory. " alt="" coords="507,461,677,488"/>
<area shape="rect" id="node19" href="$_memory_manager_8h.html#a7161fed197cb374280e918eafb4d39a9" title="function used read/write and check the serial parameters in the memory. " alt="" coords="501,411,683,437"/>
<area shape="rect" id="node4" href="$_f_m25_v20_mem_test_8h.html#a1294aa9668bfe5b70480e64ab33d5a20" title="FM25V20MemTest_Main" alt="" coords="753,132,919,159"/>
<area shape="rect" id="node11" href="$_memory_manager_8h.html#a75f5428e07dbdaee7b7d024a3447da8b" title="function use to initialize the memory manager. " alt="" coords="768,385,904,412"/>
<area shape="rect" id="node12" href="$main_8c.html#aadf3292d1b050137201649db87e63aa5" title="Function used to initialize all non critical peripheral. " alt="" coords="1143,385,1199,412"/>
<area shape="rect" id="node13" href="$main_8c.html#a6288eba0f8e8ad3ab1544ad731eb7667" title="Main function. " alt="" coords="1277,411,1328,437"/>
<area shape="rect" id="node16" href="$_usb_manager_8h.html#ac8d1502564dd3480fc417f834a13cec2" title="Function use to deal received command. " alt="" coords="757,436,915,463"/>
<area shape="rect" id="node17" href="$_usb_manager_8h.html#a1e480179c92fe988f89777f353e9ef9a" title="USB manager. " alt="" coords="969,436,1063,463"/>
<area shape="rect" id="node18" href="$main_8c.html#a47b19cb17359b8a4930e1db6207395fb" title="Function used to deal background task. " alt="" coords="1113,436,1229,463"/>
</map>
