<map id="PowerManagerExitLPM" name="PowerManagerExitLPM">
<area shape="rect" id="node2" href="$device_8c.html#a631a644dd7e158b7fa45c4bfe43b29bc" title="Function to switch the processor on the highest clock speed allowed. " alt="" coords="247,944,441,971"/>
<area shape="rect" id="node3" href="$_power_manager_8c.html#a611c841c363bb8044e88747cc39e7c30" title="power manager. " alt="" coords="290,995,398,1022"/>
<area shape="rect" id="node35" href="$_d_s_p__mkl16z256vlh4_8c.html#ad30b60ccfc1302cb250629c495851333" title="Functions to MAP the defined IO of the SPI module x in the rigth pin. " alt="" coords="1032,1091,1208,1118"/>
<area shape="rect" id="node37" href="$_power_manager_8c.html#ad82283ab9a30920f56833e7d42dd66c8" title="PowerManagerClearWakeUpInterruptFlag" alt="" coords="214,1134,474,1160"/>
<area shape="rect" id="node38" href="$_power_manager_8c.html#abc288b84841dcde78bcdb6f57da9d8d1" title="PowerManagerDisableWakeUp\lInterrupt" alt="" coords="243,1185,445,1226"/>
<area shape="rect" id="node39" href="$_d_s_p__mkl16z256vlh4_8c.html#aa0ebd2465a6d7946e08a90b6dd0dfd90" title="Functions to enable/disable the main clock of the specified uart. " alt="" coords="282,1251,406,1278"/>
<area shape="rect" id="node40" href="$_d_s_p__mkl16z256vlh4_8c.html#ade83ccc4c990b0da74572b7fbc556015" title="UART1ClockGate" alt="" coords="282,1302,406,1328"/>
<area shape="rect" id="node41" href="$_d_s_p__mkl16z256vlh4_8c.html#aaf402774cc148a8964baef5dfa2c0f63" title="UART2ClockGate" alt="" coords="282,1352,406,1379"/>
<area shape="rect" id="node42" href="$watchdog_8c.html#a81cfb9599bb68eb5f60a1c34a3c5e480" title="Kick the watchdog to avoid reset after the watchdog have started. " alt="" coords="291,1403,397,1430"/>
<area shape="rect" id="node4" href="$_b_q27510_d_r_z_r_g2_8c.html#ab6764798c058c46b3cdcf21c97027ffb" title="Function used to get all information about the cell monitoring. " alt="" coords="568,459,675,486"/>
<area shape="rect" id="node25" href="$_power_manager_8c.html#a851ecff0a5e93c3b261accadbf32621b" title="PowerManagerDisplayLoaded" alt="" coords="525,915,718,942"/>
<area shape="rect" id="node33" href="$_power_manager_8c.html#aa781287c32b2238935eb53a6ce806419" title="PowerManagerDisplayLoading" alt="" coords="523,966,719,992"/>
<area shape="rect" id="node36" href="$_power_manager_8c.html#a20ccb5a44ea9c3ecb98d6ec3ed84c62a" title="PowerManagerDisplayLoading\lError" alt="" coords="523,1017,719,1058"/>
<area shape="rect" id="node5" href="$_b_q27510_d_r_z_r_g2_8c.html#ab9dcad56c77f04971532555567a0d84b" title="Function used to know if a battery is connected or not. " alt="" coords="1040,180,1200,207"/>
<area shape="rect" id="node7" href="$_b_q27510_d_r_z_r_g2_8c.html#ac5d4fef49e298779b1753f40cf601cd3" title="BQ_getAvailableEnergy" alt="" coords="797,54,955,80"/>
<area shape="rect" id="node9" href="$_b_q27510_d_r_z_r_g2_8c.html#a9854bebed505691984f1cfa674cb3cb1" title="BQ_getAverageCurrent" alt="" coords="799,104,953,131"/>
<area shape="rect" id="node10" href="$_b_q27510_d_r_z_r_g2_8c.html#a28acfc3f3d1ff8e9d9d91edadc29ecd5" title="BQ_getAveragePower" alt="" coords="802,155,950,182"/>
<area shape="rect" id="node11" href="$_b_q27510_d_r_z_r_g2_8c.html#af8268e396eeb7abdfb21a7fbf03f1396" title="Function used to get some information about the cell monitoring. " alt="" coords="796,206,956,232"/>
<area shape="rect" id="node12" href="$_b_q27510_d_r_z_r_g2_8c.html#af6d8cc1ca065bcb90798788851de572c" title="BQ_getCellVoltage" alt="" coords="810,256,942,283"/>
<area shape="rect" id="node13" href="$_b_q27510_d_r_z_r_g2_8c.html#a02b013ae0aec405f9c7ceb909199f5f0" title="BQ_getCycleCount" alt="" coords="809,307,943,334"/>
<area shape="rect" id="node14" href="$_b_q27510_d_r_z_r_g2_8c.html#aaead900b00cb48e635c7db154f99c3e5" title="BQ_getFullAvailableCapacity" alt="" coords="781,358,971,384"/>
<area shape="rect" id="node15" href="$_b_q27510_d_r_z_r_g2_8c.html#a148f18dc993b083cacc31ff1f4dc71ed" title="BQ_getFullChargeCapacity" alt="" coords="787,408,965,435"/>
<area shape="rect" id="node16" href="$_b_q27510_d_r_z_r_g2_8c.html#a42dac1127d0914053de05fd9af45b77a" title="BQ_getMaxLoadCurrent" alt="" coords="795,459,957,486"/>
<area shape="rect" id="node17" href="$_b_q27510_d_r_z_r_g2_8c.html#aa723c8cc7b39b74ae4c344cb39350aed" title="BQ_getMaxLoadTimeToEmpty" alt="" coords="777,510,975,536"/>
<area shape="rect" id="node18" href="$_b_q27510_d_r_z_r_g2_8c.html#a14b533c028c320fc9b2a5b9043d0e259" title="BQ_getNominalAvailableCapacity" alt="" coords="769,560,983,587"/>
<area shape="rect" id="node19" href="$_b_q27510_d_r_z_r_g2_8c.html#a6602062ce84e9142bfab316784516eb8" title="BQ_getRemainingCapacity" alt="" coords="787,611,965,638"/>
<area shape="rect" id="node20" href="$_b_q27510_d_r_z_r_g2_8c.html#a3a21f0765f44c716b638d8b8773946d2" title="BQ_getStandbyTimeToEmpty" alt="" coords="779,662,973,688"/>
<area shape="rect" id="node21" href="$_b_q27510_d_r_z_r_g2_8c.html#a84d862a65a34dff063b11338b89a5931" title="BQ_getStateOfCharge" alt="" coords="801,712,951,739"/>
<area shape="rect" id="node22" href="$_b_q27510_d_r_z_r_g2_8c.html#ab0c39d16ad675e6a83e2659c9a51551b" title="BQ_getTimeToEmpty" alt="" coords="803,763,949,790"/>
<area shape="rect" id="node23" href="$_b_q27510_d_r_z_r_g2_8c.html#aade4e442c60a3cf1aa9223a7696483dc" title="BQ_getTimeToFull" alt="" coords="811,814,941,840"/>
<area shape="rect" id="node24" href="$_b_q27510_d_r_z_r_g2_8c.html#a8a62d091a91f6665acc0bd38ee9af9da" title="BQ_getTTEAtConstantPower" alt="" coords="781,864,971,891"/>
<area shape="rect" id="node6" href="$i2c0_8c.html#ada7d730a8793a6ddd23180047b309447" title="Send a packet on the I2C interface. " alt="" coords="1257,307,1335,334"/>
<area shape="rect" id="node8" href="$i2c0_8c.html#a1f3862c3506c31b0a50c7914f17314ab" title="Read a packet on the I2C interface. " alt="" coords="1081,434,1159,460"/>
<area shape="rect" id="node26" href="$display_8c.html#ad8f9098d6f81dbce9ff70ef99662f212" title="Function used get the data displayed. " alt="" coords="791,915,961,942"/>
<area shape="rect" id="node27" href="$display_8c.html#a0529c896e4069df4bb7c4e767f36be28" title="Function used set the data displayed. " alt="" coords="791,966,961,992"/>
<area shape="rect" id="node28" href="$decoder16_seg_8c.html#a2d2fc41a03a66256e4681e8d695f01b0" title="Function used to decode a char and display it on a 16 segments digit. " alt="" coords="1040,814,1200,840"/>
<area shape="rect" id="node29" href="$decoder7_seg_8c.html#a8e8cab35cf7c9517f7094f42637a086e" title="Function used to decode a char and display it on a 7 segments digit. " alt="" coords="1043,864,1197,891"/>
<area shape="rect" id="node30" href="$display_8c.html#a771439bf50110fb999649ac3262bc4ef" title="Function used to root 16 segments command on the rigth PIN. " alt="" coords="1049,915,1191,942"/>
<area shape="rect" id="node31" href="$display_8c.html#ace411722dfe7b549d16c09991a5ff24f" title="Function used to root 7 segments command on the rigth PIN. " alt="" coords="1053,966,1187,992"/>
<area shape="rect" id="node32" href="$spi0_8c.html#a6d528a26e3df5e8bdb80622df3946998" title="Function used to send data over the SPI module 0. " alt="" coords="1081,1040,1159,1067"/>
<area shape="rect" id="node34" href="$display_8c.html#a20d8e5860540ecfe3c0bb5a237bc17f8" title="Function used to enable/disable the display power. " alt="" coords="815,1024,937,1051"/>
</map>
