<map id="FM25V20_SetWriteEnable" name="FM25V20_SetWriteEnable">
<area shape="rect" id="node2" href="$_f_m25_v20_8h.html#a69f76e4332c185e885cdc6691bb075c2" title="Functions used to set and read the status register. " alt="" coords="230,107,389,133"/>
<area shape="rect" id="node7" href="$_f_m25_v20_8h.html#a614bc8a001d6845b564f529dc542410d" title="Write data to the memory. " alt="" coords="241,259,377,285"/>
<area shape="rect" id="node3" href="$_f_m25_v20_8h.html#a2e18e393748dca1da43e4e069bc4972f" title="Function used to initialize the FM25V20 memory. " alt="" coords="502,5,597,32"/>
<area shape="rect" id="node4" href="$_memory_manager_8h.html#a75f5428e07dbdaee7b7d024a3447da8b" title="function use to initialize the memory manager. " alt="" coords="725,56,861,83"/>
<area shape="rect" id="node5" href="$main_8c.html#aadf3292d1b050137201649db87e63aa5" title="Function used to initialize all non critical peripheral. " alt="" coords="1116,284,1172,311"/>
<area shape="rect" id="node6" href="$main_8c.html#a6288eba0f8e8ad3ab1544ad731eb7667" title="Main function. " alt="" coords="1251,348,1301,375"/>
<area shape="rect" id="node8" href="$_f_m25_v20_mem_test_8h.html#a4fa08b2f438caece8e0907091a74496f" title="FM25V20MemTest_Set" alt="" coords="470,56,629,83"/>
<area shape="rect" id="node10" href="$_f_m25_v20_mem_test_8h.html#a31b1c7bd95f8fc629c82fedbc7e86c19" title="FM25V20MemTest_Clear" alt="" coords="465,107,634,133"/>
<area shape="rect" id="node11" href="$_f_m25_v20_mem_test_8h.html#a3dab3a8f4d5b585ffc341132a8905a4e" title="FM25V20MemTest_HighFreqUp" alt="" coords="446,157,653,184"/>
<area shape="rect" id="node12" href="$_f_m25_v20_mem_test_8h.html#a5324c46da6daa18c72d434ddd2695b87" title="FM25V20MemTest_HighFreqDown" alt="" coords="438,208,661,235"/>
<area shape="rect" id="node13" href="$_f_m25_v20_mem_test_8h.html#a5a0a75083ba30546c433ecb0b12edf3d" title="FM25V20MemTest_PulseP" alt="" coords="459,259,640,285"/>
<area shape="rect" id="node14" href="$_f_m25_v20_mem_test_8h.html#aa801df1c3fb82c4b63ea3da6209ac73d" title="FM25V20MemTest_PulseN" alt="" coords="459,309,640,336"/>
<area shape="rect" id="node15" href="$_memory_manager_8h.html#afff43e62869a6852a9b8e7c5c8683e25" title="function used read/write and check the diving parameters in the memory. " alt="" coords="457,360,641,387"/>
<area shape="rect" id="node19" href="$_memory_manager_8h.html#a45e7b71d057b396d37a5867806284b40" title="function used read/write and check the serial parameters in the memory. " alt="" coords="458,411,641,437"/>
<area shape="rect" id="node20" href="$_memory_manager_8h.html#aaf68fcb13458866a83fe16fa9c66aca9" title="function used read/write and check the log in the memory. " alt="" coords="464,512,635,539"/>
<area shape="rect" id="node23" href="$_memory_manager_8h.html#aa72a3e9863e2ac9b476266b1fad21575" title="function used read/write and check the log in the memory. " alt="" coords="464,461,635,488"/>
<area shape="rect" id="node9" href="$_f_m25_v20_mem_test_8h.html#a1294aa9668bfe5b70480e64ab33d5a20" title="FM25V20MemTest_Main" alt="" coords="710,183,877,209"/>
<area shape="rect" id="node16" href="$_usb_manager_8h.html#ac8d1502564dd3480fc417f834a13cec2" title="Function use to deal received command. " alt="" coords="714,411,873,437"/>
<area shape="rect" id="node17" href="$_usb_manager_8h.html#a1e480179c92fe988f89777f353e9ef9a" title="USB manager. " alt="" coords="934,411,1029,437"/>
<area shape="rect" id="node18" href="$main_8c.html#a47b19cb17359b8a4930e1db6207395fb" title="Function used to deal background task. " alt="" coords="1086,411,1202,437"/>
<area shape="rect" id="node21" href="$_button_manager_8c.html#afdd019b240e44a51aba9069b09cd3ee8" title="ButtonManagerDealer" alt="" coords="720,499,867,525"/>
<area shape="rect" id="node22" href="$_button_manager_8h.html#a6131a6127b6045f5c352ca091ebdb36a" title="Button manager function. " alt="" coords="926,487,1037,513"/>
</map>
