<map id="PowerManagerDisplayLoaded" name="PowerManagerDisplayLoaded">
<area shape="rect" id="node2" href="$display_8c.html#ad8f9098d6f81dbce9ff70ef99662f212" title="Function used get the data displayed. " alt="" coords="248,56,419,83"/>
<area shape="rect" id="node3" href="$display_8c.html#a0529c896e4069df4bb7c4e767f36be28" title="Function used set the data displayed. " alt="" coords="249,107,418,133"/>
<area shape="rect" id="node4" href="$decoder16_seg_8c.html#a2d2fc41a03a66256e4681e8d695f01b0" title="Function used to decode a char and display it on a 16 segments digit. " alt="" coords="467,5,627,32"/>
<area shape="rect" id="node5" href="$decoder7_seg_8c.html#a8e8cab35cf7c9517f7094f42637a086e" title="Function used to decode a char and display it on a 7 segments digit. " alt="" coords="470,56,623,83"/>
<area shape="rect" id="node6" href="$display_8c.html#a771439bf50110fb999649ac3262bc4ef" title="Function used to root 16 segments command on the rigth PIN. " alt="" coords="475,107,618,133"/>
<area shape="rect" id="node7" href="$display_8c.html#ace411722dfe7b549d16c09991a5ff24f" title="Function used to root 7 segments command on the rigth PIN. " alt="" coords="479,157,614,184"/>
<area shape="rect" id="node8" href="$spi0_8c.html#a6d528a26e3df5e8bdb80622df3946998" title="Function used to send data over the SPI module 0. " alt="" coords="507,232,586,259"/>
</map>
