<map id="WatchdogKick" name="WatchdogKick">
<area shape="rect" id="node2" href="$_c_r95_uart_mapper_8h.html#a530fdd7929335f4103bf44a111d9f441" title="CR95HF Uart interface. " alt="" coords="225,285,319,311"/>
<area shape="rect" id="node5" href="$main_8c.html#aadf3292d1b050137201649db87e63aa5" title="Function used to initialize all non critical peripheral. " alt="" coords="871,225,927,251"/>
<area shape="rect" id="node6" href="$main_8c.html#a6288eba0f8e8ad3ab1544ad731eb7667" title="Main function. " alt="" coords="1005,437,1056,463"/>
<area shape="rect" id="node7" href="$main_8c.html#a040d63354f4112c7ec2ca4d3a86a5b4a" title="Function used to initialize some critical peripheral. " alt="" coords="859,538,938,565"/>
<area shape="rect" id="node8" href="$_f_m25_v20_mem_test_8h.html#a31b1c7bd95f8fc629c82fedbc7e86c19" title="FM25V20MemTest_Clear" alt="" coords="187,639,357,666"/>
<area shape="rect" id="node10" href="$_f_m25_v20_mem_test_8h.html#a5324c46da6daa18c72d434ddd2695b87" title="FM25V20MemTest_HighFreqDown" alt="" coords="161,386,383,413"/>
<area shape="rect" id="node11" href="$_f_m25_v20_mem_test_8h.html#a3dab3a8f4d5b585ffc341132a8905a4e" title="FM25V20MemTest_HighFreqUp" alt="" coords="169,437,375,463"/>
<area shape="rect" id="node12" href="$_f_m25_v20_mem_test_8h.html#aa801df1c3fb82c4b63ea3da6209ac73d" title="FM25V20MemTest_PulseN" alt="" coords="181,487,363,514"/>
<area shape="rect" id="node13" href="$_f_m25_v20_mem_test_8h.html#a5a0a75083ba30546c433ecb0b12edf3d" title="FM25V20MemTest_PulseP" alt="" coords="181,538,363,565"/>
<area shape="rect" id="node14" href="$_f_m25_v20_mem_test_8h.html#a4fa08b2f438caece8e0907091a74496f" title="FM25V20MemTest_Set" alt="" coords="193,589,351,615"/>
<area shape="rect" id="node15" href="$_memory_manager_8h.html#aa72a3e9863e2ac9b476266b1fad21575" title="function used read/write and check the log in the memory. " alt="" coords="187,791,357,818"/>
<area shape="rect" id="node19" href="$_memory_manager_8h.html#a95c0f9ae110105c19fb6eb0da09930e0" title="Return the number of log stored in memory. " alt="" coords="166,133,378,159"/>
<area shape="rect" id="node20" href="$_memory_manager_8h.html#a75f5428e07dbdaee7b7d024a3447da8b" title="function use to initialize the memory manager. " alt="" coords="460,183,596,210"/>
<area shape="rect" id="node21" href="$_memory_manager_8h.html#a4dd1d910cde969a31ad009fcca1bb4a4" title="function used read/write and check the diving parameters in the memory. " alt="" coords="181,234,363,261"/>
<area shape="rect" id="node22" href="$_memory_manager_8h.html#a4621c0be0193d08ee84b8dc8bdaea778" title="function used read/write and check the log in the memory. " alt="" coords="187,842,357,869"/>
<area shape="rect" id="node23" href="$_memory_manager_8h.html#a7161fed197cb374280e918eafb4d39a9" title="function used read/write and check the serial parameters in the memory. " alt="" coords="181,82,363,109"/>
<area shape="rect" id="node24" href="$_memory_manager_8h.html#afff43e62869a6852a9b8e7c5c8683e25" title="function used read/write and check the diving parameters in the memory. " alt="" coords="180,893,364,919"/>
<area shape="rect" id="node25" href="$_memory_manager_8h.html#aaf68fcb13458866a83fe16fa9c66aca9" title="function used read/write and check the log in the memory. " alt="" coords="187,741,357,767"/>
<area shape="rect" id="node28" href="$_memory_manager_8h.html#a45e7b71d057b396d37a5867806284b40" title="function used read/write and check the serial parameters in the memory. " alt="" coords="181,943,363,970"/>
<area shape="rect" id="node29" href="$_power_manager_8h.html#a7406ccf39ad8768c5043ac74da94a63b" title="Functions used to Enter and exit low power mode. " alt="" coords="189,1045,355,1071"/>
<area shape="rect" id="node31" href="$_power_manager_8h.html#a1c56b577113fb8580a4f6fb0abe50fea" title="Functions used to Enter and exit low power mode. " alt="" coords="193,994,351,1021"/>
<area shape="rect" id="node3" href="$_c_r95_h_f_8h.html#a5a280da3bb75613fbb5e62854ec65e3a" title="Function used to initialize the CR95HF global manager. " alt="" coords="484,259,572,286"/>
<area shape="rect" id="node4" href="$_r_f_i_d_manager_8h.html#a67c55a98971bdbdc992fd3c60daebcc8" title="Function used to initialize the RFID manager. " alt="" coords="673,253,791,279"/>
<area shape="rect" id="node9" href="$_f_m25_v20_mem_test_8h.html#a1294aa9668bfe5b70480e64ab33d5a20" title="FM25V20MemTest_Main" alt="" coords="445,513,611,539"/>
<area shape="rect" id="node16" href="$_usb_manager_8h.html#ac8d1502564dd3480fc417f834a13cec2" title="Function use to deal received command. " alt="" coords="449,842,607,869"/>
<area shape="rect" id="node17" href="$_usb_manager_8h.html#a1e480179c92fe988f89777f353e9ef9a" title="USB manager. " alt="" coords="685,817,779,843"/>
<area shape="rect" id="node18" href="$main_8c.html#a47b19cb17359b8a4930e1db6207395fb" title="Function used to deal background task. " alt="" coords="841,810,957,837"/>
<area shape="rect" id="node26" href="$_button_manager_8c.html#afdd019b240e44a51aba9069b09cd3ee8" title="ButtonManagerDealer" alt="" coords="455,753,601,779"/>
<area shape="rect" id="node27" href="$_button_manager_8h.html#a6131a6127b6045f5c352ca091ebdb36a" title="Button manager function. " alt="" coords="677,759,787,786"/>
<area shape="rect" id="node30" href="$_power_manager_8h.html#aef7050cf231cfdbbdb4134de79e10add" title="Low Power mode controller. " alt="" coords="433,994,623,1021"/>
</map>
